# Server-only Configuration on the Network LAN

In this configuration, the server is installed in the customer’s existing network LAN with no exposure to the Internet.

Some examples of deployments that use this configuration are:

- Secure Call Recording

- Daisy Chaining

- MiCollab remote management (see also the MiCollab Example)

#### MSL Configuration

In MSL, do the following:

1. Access the MSL Server Console and select Configure this server.

2. In Local Network Parameters, enter the server's internal (LAN) IP address server or select the default. This address SHOULD be:

- dedicated to the MBG solution

- private

- reachable only from the internal network

#### MBG Configuration

In MBG, do the following:

1. On the MBG main page, click the System configuration tab and then click Network profiles.

2. Select Server-only configuration on the network LAN.

3. Select Apply LAN configuration.

When configuration is complete, the system will use the LAN address of the server for both the set-side and ICP-side streaming addresses of the MBG.

The following diagram provides an example of a "Server-only configuration on the network LAN":