# MiVoice 5000, MiVoice MX-ONE, and MiVoice Office 400 Network Element Field Descriptions

Field | Description | Values
Type | Select network element type required. Mandatory. | MiVoice Business, MiVoice 5000, MiVoice MX-ONE Service Node, or MiVoice Office 400.
System Name | Enter the unique network element name. For example, "MiV5000_3". Mandatory. This field is read-only for the local MiCollab Server network element. | Enter a unique name of between two and 64 characters in length for the network element. The name can consist of alphanumeric and certain special characters. Spaces are allowed.
IP Address | Enter the IP address of the network element. Mandatory. This field is read-only for the local MiCollab Server network element. Note: For MiVoice MX-ONE deployments, enter the IP address of the MX-ONE Service Node Manager. | Standard IP address notation of four sets of one to three digits separated by periods. For example, 192.168.0.1
Zone | Enter a number to identify the Network Zone. | Number from 1 to 999. Default is blank.
FQDN | Enter a Fully Qualified Domain Name for the network element. | Optional
Outgoing Dialing Prefix | Enter the outgoing dialing prefix to be used by MiCollab Client. | Enter a number up to 32 digits in length. Valid digits are 0 to 9. This field is optional.
Call Forward Destination Directory Number | Enter the NP-UM voice mail number to be used by MiCollab Client. | 10-digit number maximum.
SIP Conference FAC: | This field defines the Feature Access Code that MiCollab Client users dial to establish a 3-party conference. The system copies the code from this field to the PBX Node details page of the MiCollab Client Service. Note: This FAC does not apply to MiVoice Office 250 or MiVoice Office 400 platforms. A FAC is not used to establish 3-party conferences on these communication platforms. | MiVoice 5000 default is *40. MiVoice MX-ONE default is 3. Limit of 16 telephony characters (0-9, *, #)