# MiVoice Business Network Element Field Descriptions

Field | Description | Values
Type | Select the PBX type. Mandatory. | MiVoice Business, MiVoice 5000, MiVoice MX-ONE Service Node, or MiVoice Office 400. Note: The MiVoice Business system identifies a MiCollab Server as Type "MSL Server" in the system administration tool.
System Name | Enter the unique network element name. For example, "MiVB3". Mandatory. This field is read-only for the local MiCollab Server network element. | Enter a unique name of between two and eight characters in length for the network element. The name can consist of alphanumeric and certain special characters. Spaces are not allowed.
IP Address | Enter the IP address of the network element. Mandatory. T his field is read-only for the local MiCollab Server network element | Mandatory. Standard IP address notation of four sets of one to three digits separated by periods. For example, 192.168.0.1
Zone | Enter a number to identify the Network Zone. The MiVoice Business platform uses Network Zones for compression and bandwidth management to associate the zones to time zones for the display of local time on IP sets to configure the zone's Location Based Number (LBN) prefix for Location Base Call Routing (optional), and to define the zone's CESID (optional). | Number from 1 to 999. Default is blank. If this field is left blank, the MiVoice Business defaults this setting to Zone 1.
FQDN | Enter a Fully Qualified Domain Name for the MiVoice Business network element. Optional. | Optional

### Network Element Settings

Field | Description | Values
SIP Conference FAC: | If MiCollab Client is in integrated mode, this field defines the Feature Access Code that MiCollab Client users dial to establish a 3-party conference. If MiCollab Client is in integrated mode, the system copies the code from this field to the PBX Node details page of the MiCollab Client Service. If MiCollab Client is in co-located mode, this field is not used and you must enter the code in the PBX Node details page. This field is not shared via Flow Through Provisioning. | Default is *40. Limit of 16 telephony characters (0-9, *, #)

### Credentials

Field | Description | Values
System Login | Enter the MiVoice Business System Administration Tool Login ID. This field is mandatory. | Up to 20 alphanumeric characters. Must be a valid Login ID for a MiVoice Business user profile with Application access.
Password | Enter the password associated with the MiVoice Business System Administration Tool Login ID. This field is mandatory. | MiVoice Business password. Note: Ensure that you enter the MiVoice Business System Login and Password correctly. If either are incorrect, users will be unable to change their Telephone User Interface (TUI) passcodes.
Confirm Password | Re-enter the password to confirm. |

### System Properties

Note: If you create a new MiVoice Business network element in the MiVoice Business cluster and start sharing it with MiCollab, you must add the element's Set Registration Code and Set Replacement Code in these fields, because SDS does not share them with MiCollab.

Field | Description | Values
Set Registration Code | Enter an access code to register a new IP telephone into the system. The access code consists of digits to add at the beginning of a PIN when registering an IP telephone. | May be 3 to 10 digits in length, including * or # (for example: ###). Cannot be the same as Set Replacement Code.
Set Replacement Code | Enter an access code to override an already registered IP telephone. The access code consists of digits to add at the beginning of a PIN when registering an IP telephone. | May be 3 to 10 digits in length, including * or # (for example: ***). Cannot be the same as Set Registration Code.
Use NuPoint UM IP Integration Licenses | If the Network Element will support the NuPoint UM application ports select this check box. After you click Save, the Network Element (ICP) is configured in the NuPoint UM application. You must activate this change in the NuPoint UM application from the activation link at the top of the page. |

### Application Data

#### Voicemail

Field | Description | Values
Call Reroute First Alternative (CRFA) Number | This setting allows you to configure call rerouting for devices at the system level. Enter the CRFA index number for call rerouting. Ensure that a destination extension (for example, voice mail hunt group number) is programmed against the index number in the Call Reroute First Alternative form of the MiVoice Business platform. | Number from 1 to 336 digits in length. When you create a phone with a mailbox, or add a mailbox to an existing phone, the system automatically applies the CRFA programming to the device. Note: Prior to MiCollab Release 6.0, Call Forwarding was used to direct calls to the voice mail hunt group number. Call Forwarding takes precedence over CRFA. Defaults to Call Reroute First Alternative index number 2 with the voice mail hunt group number set to extension 7000.
Call Forward Destination Directory Number | Enter the NP-UM voice mail hunt group number to be used by MiCollab Client. | 7-digit number maximum. (Default applied by MiCW is 7000).
HCI Reroute Hunt Group Number for MiTai MWI | Enter the hunt group number for the HCI Reroute Hunt Group. (This hunt group is used to enable MWI lamp on stations with mailboxes via the MiTAI application interface.) | 7-digit number maximum. (Default applied by MiCW is 6400).

#### Speech Auto Attendant

Field | Description | Values
Pilot/Access Number | Enter the pilot number of the Speech Auto Attendant (SAA). This number is listed in the Welcome E-mail that the system sends to new users. For MiVoice Business systems, enter the "Speech Auto Attendant" Hunt Group directory number that is listed in the Telephone Directory form of the System Administration Tool. Note: MiCollab does not verify that the entered number is a valid entry in the MiVoice Business database. Note: This field is only present if the SAA application is licensed and installed on MiCollab. | 7-digit number maximum. (Default applied by MiCW is 6800).