# Overview of Network Profiles

MBG provides some preset streaming address configurations that you can choose according to your network profile (configuration setup). In most cases, you can select the network profile that applies to your particular configuration. In some situations, however, the preset defaults may not be appropriate. In those cases, you can enter a custom configuration with manually entered Set-side and ICP-side IP addresses.

The default settings provided with the presets are as follows:

Network Profile | Default Set Side IP Address for RTP Streaming | Default ICP Side IP Address for RTP Streaming
Server-gateway on network edge | WAN IP address | LAN IP address
Server-only on network DMZ | Public IP address as seen by the AMC | Public IP address as seen by the AMC
Server-only on network LAN | LAN IP address | LAN IP address

Note: Improper selection of network profile can result in calls that have one-way audio or no audio at all.

## Network Profiles

- Server Gateway on the Network Edge

- Server-only on the Network DMZ

- Server-only on the Network LAN

- Server Gateway with Bridged Interface

## Daisy Chain Mode

Daisy chaining MBG servers provides a method of decreasing the virtual distance by allowing local streaming access among remote offices. For configuration details, see the MBG Installation and Maintenance Guide.

To put the server into Daisy Chain mode:

1. On the MBG main page, click the System configuration tab and then click Network profiles.

2. Click Enter Daisychain Mode.

3. In the Daisy-chain IP address field, enter the IP address of the upstream MBG server.

4. Click Save.