# Configuration Quick Reference

## Description

Basic configuration of the NuPoint Unified Messaging system consists of assigning groups of telephone lines (called "line groups") to the applications that will handle the following:

- incoming calls (NuPoint Voice application)

- outdialing (Pager application)

- message waiting indication (MWI application)

## Configuration

### Set Up a Line Group for Incoming Calls on MiVoice Business ICP Systems

Setting up an incoming line group consists of the following tasks:

- configure the ICP integration

- configure the ICP line group

- map extension numbers (ports) to triplets (in this example, we will map ports 1 -7 (1:0:0 to 1:0:6) to extensions 3301 to 3307

To set up an incoming line group:

1. Log in to the console as "root".

2. From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, (R) Reconfigure System, (G) Offline Menu, and then (B) Duplicate Offline Configuration.

3. Select (I) Server Options and configuration.

4. Select (C) Configure Mitel MCD Integration.

5. Map the MiVoice Business ICP integration by entering the following configuration information. Note that each of the following entries must match the information entered in the MiVoice Business ICP System Option form.

6. (N) The name of MiVoice Business ICP server to be configured for integration with the NuPoint Unified Messaging server, for example, [pbx3].

7. (I) The Mitel MCD address or FQDN to which you are mapping, for example [10.37.237.150] or [pbx4.mitel.com].

8. (S) The set registration code that matches with the code entered in the System Options form on the MiVoice Business ICP, for example, [***].

9. (R) The set replacement code that matches with the code entered in the System Options form on the MiVoice Business ICP, for example, [###].

5. Exit the MiVoice Business Integration Menu and then exit the Server Options Configuration Menu.

6. In the Offline Configuration Menu, select (G) Define Line Groups, Fax Groups.

7. Define the line group by entering the following configuration information:

8. (N) Name of current group, for example, [Incoming Line Group].

9. (A) Add lines to current group, in this example, we will add [1:0:0-1:0:6]

8. Select (M) Mapping Extension/Port, (E) Map Extension Number for ICP, and then (P) Port Mapping.

9. Enter the extension number: in this example, we want to assign extensions 3301 to 3307 [3301-3307] to the selected triplets.

10. Exit the offline menu to save your changes to the offline configuration.

If you are finished making offline changes, select (A) to Activate the Offline Configuration. If you have more changes to make, exit to the Main Menu.

### Set Up a Line Group for Paging/Outdialing

In this example, we will support an Internal paging system (0) and an External paging system (1) and we will map port 1:0:7 to extension 3008.

1. From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, (R) Reconfigure System, (G) Offline Menu, and then (B) Duplicate Offline Configuration.

2. Select (I) Server options and configuration.

3. Select (C) Configure ICP Integration.

4. Map the MiVoice Business ICP integration by entering the following configuration information. Note that each of the following entries must match the information entered in the MiVoice Business ICP System Option form.

5. (N) The name of MiVoice Business ICP server to be configured for integration with the NuPoint Unified Messaging server, for example, [pbx3].

6. (I) The ICP IP address to which you are mapping, for example [10.37.237.150].

7. (S) The set registration code that matches with the code entered in the System Options form on the MiVoice Business ICP, for example, [***].

8. (R) The set replacement code that matches with the code entered in the System Options form on the MiVoice Business ICP, for example, [###]

5. Exit the MiVoice Business Integration Menu and then exit the Server Options Configuration Men.

6. In the Offline Configuration Menu, select (G) Define Line Groups, Fax Groups.

7. Define the line group by entering the following configuration information:

8. (N) Name of current group, for example, [Incoming Line Group]

9. (A) Add lines to current group, in this example, we will add [1:0:0-1:0:6]

8. Select (M) Mapping Extension/Port, (E) Map Extension Number for ICP, and then (P) Port Mapping.

9. Enter the extension number: in this example, we want to assign extensions 3301 to 3307 [3301-3307] to the selected triplets.

10. Exit the offline menu to save your changes to the offline configuration.

If you are finished making offline changes, select (A) to Activate the Offline Configuration. If you have more changes to make, exit to the Main Menu.

### Set Up a Line Group for Message Waiting Indication