# Category 21: Paging and Message Delivery Feature Bits

These feature bits control paging and message delivery options. Some of these feature bits allow a user to override a default schedule or pager number. Set up the Pager application to use these feature bits. Cut-through Paging is an optional feature.

Bit | Description | Required | Incompatible
077 | Change pager schedule | 070 |
079 | Set message wait #1 for urgent messages only | 040, 041, 088 | 080, 228
080 | Set message wait #2 for urgent messages only | 040, 041, 088 | 079, 228
124 | Change paging phone number |  | 070
163 | Don’t play message count |  | 40-45, 88, 175, 179
168 | Message wait 1, pager requeue |  |
169 | Message wait 2, pager requeue |  |
171 | Cut-through Paging | 070 |
172 | Cut-through Paging and messaging | 070 |
173 | Receive cut-through page notify receipt | 070, 075, 171 or 172 |
181 | Paging over message delivery, message waiting 1 over message waiting 2 | 070, 077 |
188 | Append # to end of cut-through page number | 070, 171 or 172 |
208 | Play reorder tone after CTP or greet-only | 171 or 172 |
209 | Tone only pager interface |  |
210 | Numeric display pager mailbox interface |  |
211 | Voice pager mailbox interface |  |
212 | Send page upon answer, greet-only mbox |  |
213 | Edit CTP number with * key if no caller menu | 171 or 172 | 005
219 | Login with 0 using cut-through paging | 171 or 172 |
228 | Set msg wait #3 for urgent msgs only | 040 and/or 041, and 088 | 079, 080