# External Application (RS232) Programmable Application Parameters

Parameter | Description | Value
Programmable Parameters
Initialization String | Enter the ASCII string required by the PBX. To create the string, consult the PBX operating manual or the PBX vendor for the correct code. | 0-30 characters
Reply String | Enter the ASCII string sent by the PBX. | 0-30 characters
Delay between requests | Enter the time to wait between requests. | 0 - 255 seconds
Pre-DN ON string | If the PBX requires the string before the directory number (sometimes called extension number), create an ASCII string . If the PBX sends the string after the directory number: - enter a period (.) to delete an existing string, if necessary. - enter values for the Post-DN ON String and Post-DN OFF String parameters. | 0-30 characters
Pre-DN OFF string
Post-DN ON string | If the PBX requires the string before the directory number (sometimes called extension number), create an ASCII string . If the PBX sends the string after the directory number: - enter a period (.) to delete an existing string, if necessary. - enter values for the Post-DN ON String and Post-DN OFF String parameters. | 0-30 characters
Post-DN OFF string
Department Code as DN | Select this check box to use the department code instead of the mailbox extension as the DN to turn lights on/off. |
Unplayed Number Sent | Select this check box to send the number of unplayed messages currently in a mailbox to be included after the mail-box number.
Delay after Post-DN String | Enter the time to wait between Post-DN and Trailing String. | 0 - 255 seconds
Ending Trailing String | If the PBX requires this string, create an ASCII string If the PBX does not require this string, enter a period (.) to delete an existing string. | 0-30 characters
Suppress Updates to MWL | Select this check box to suppress updates of MWL after a user accesses the mailbox without changing status. |
Modem Result Code | This modem result code will be used to compare against the actual result code returned from the modem after it has finished outdialing the MWI string. If they are not matched, NuPoint Voice will retry the MWI request again later on. Recommendation: For *better display* of CDR events, please turn OFF the Local Echo mode of the modem, ie. if the modem has dialed a MWI string like "ATDT*13658", it should not echo back this same string prior to returning the result code. If event messages for modem dial result are desired, enable "Pager" CDR in the Event Recorder menu. | See Valid String Characters table below.
Connection Settings |
IP Address | Enter the IP address of the remote system. | (Used for PMS configuration)
Server Port Number | Enter the port that the remote device/system is listening on.

## Valid String Characters

Character | Explanation
\b | Backspace
\f | Form Feed
\n | New Line
\r | Carriage Return
\t | Tab
\\ | Backslash
\" | Double Quotes
\? | Question Mark