# Virtual Application Default Configurations

If you receive an alarm indicating that your resource dimensions are "unsupported," you can you can restore the default allocation and reservation limits settings to your virtual application. In most cases, your resource dimensions will then be "supported."

The following table lists the default allocation and reservation settings for all of the Mitel virtual applications. For configuration details, refer to the product documentation.

Mitel Border Gateway
Deployment | Ports | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
Small Business | 150 | 1 GB | 1 GB | 1 vCPUs | 1000 MHz | 20 GB | 15 GB
Enterprise | 500 | 2 GB | 2 GB | 3 vCPUs | 3000 MHz | 40 GB | 35 GB
NuPoint Unified Messenger
Deployment | Ports | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
Small Business | 60 | 4 GB | 4 GB | 2 vCPUs | 2000 MHz | 130 GB | 125 GB
Enterprise | 120 | 6 GB | 6 GB | 4 vCPUs | 4000 MHz | 260 GB | 255 GB
MiCollab
Deployment | Users | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
Small Business | 150 | 4 GB | 4 GB | 2 vCPUs | 2000 MHz | 45 GB | 40 GB
Enterprise | 1000 | 6 GB | 6 GB | 4 vCPUs | 4000 MHz | 85 GB | 80 GB
Mitel Communication Director
Deployment | Users | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
Small Business | 150 | 1.5 GB | 1.5 GB | 2 vCPUs | 1000 MHz | 20 GB | 15 GB
Mid-Enterprise | 1500 | 2.0 GB | 2.0 GB | 3 vCPUs | 3000 MHz | 20 GB | 15 GB
Enterprise | 2500 | 2.0 GB | 2.0 GB | 4 vCPUs | 5000 MHz | 20 GB | 15 GB
Unified Communicator Advanced
Deployment | Users | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
All deployments | 2000 | 2 GB | 2 GB | 2 vCPUs | 2000 MHz | 30 GB | 25 GB
Open Integration Gateway
Deployment | Ports | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
All deployments | 100 | 4 GB | 4 GB | 2 vCPUs | 2000 MHz | 20 GB | 15 GB
UCC
Deployment | Ports | Memory | vCPU | Disk Size
Allocated | Reserved | Allocated | Reserved | Allocated | Used
All deployments |  | 6 GB | 6 GB | 2 vCPUs | 2000 MHz | 40 GB | 35 GB