# Add or Edit MiNet Devices

Note: MiCollab deployments should use the MiCollab Users and Services Provisioning application for adding or editing devices.

MiNET Device Options
Field | Description | Notes
Enabled | Select to enable the set and allow it to connect to the ICP. Clear the check box to disable access. |
Configured ICP | Select a default ICP to assign to this device. |
MAC Address | Enter the MAC address of the phone manually, if required. | If the installer password is enabled on the Service configuration > ICPs tab, the device connects on its first attempt and you are prompted to enter the install password. The device appears on the Services > MiNet devices tab as Enabled, with default values, and is added to the ICP associated with that installer password. If the installer password is not enabled and an unregistered remote device attempts to connect, the server automatically registers the MAC address and configures the device as "Disabled". You must modify the appropriate Device ID and select the Enabled check box to allow access for that device. You can add a device to the list by manually entering the MAC address before deploying the device.
Description | Enter a text description for the set. | Alphanumeric entry. Maximum 256 digits.
Force set-side codec | In order to reduce the amount of bandwidth consumed on the Internet side of the connection, you can select the compression codec to apply to the voice traffic going to the remote MiNET set. Disabled to allow the selected remote device to select the codec. G.729a to force the selected remote device to use G.729 A-law. G.711u to force the selected remote device to use G.711 μ-law. G.711a to force the selected remote device to use G.711 A-law. Note: Not supported for MiCollab deployments. | Default is Use master setting.
Codec support | If you are doing secure call recording and the 3rd-party call recording equipment (CRE) only supports G.711a, G.711u and G.729a, you can restrict MBG to using those codecs. If you are not operating under these limitations, you should allow MBG to use an unrestricted range of codecs. Unrestricted to the selected remote device to use any codec. Restricted to G.729, G.711 to force the selected remote device to use G.711a, G.711u, or G.729a. | Default is Use master setting.
Local Streaming | Select a local streaming option: Always to force the remote device to use local streaming always. Never to prevent the remote device from using local streaming. | Default is Use master setting.
Log verbosity |  | Default is Use master setting.
Log to individual file | This option enables you to collect log files for the selected remote device, which enables you to isolate and troubleshoot problems being experienced by a particular user. Select the check box to generate the following log files: Current log file All log files (zipped) The device-level log files are available for downloading from the View Log Files panel in the MSL Server Manager. See tug/devices. | Default is disabled.
Enable Detailed Jitter Log | Similar to log verbosity, this field controls the jitter log. Enabled to enable detailed logging for the selected device Disabled to disable detailed logging for the selected device | Default is Use master setting.
RTP Framesize | This setting overrides the default value requested by the ICP or SIP peer request. It should be changed only if your system has specific requirements. For more information about RTP frame size, see the Engineering Guidelines. | Default is Use master setting.
Disable SRTP | If SRTP is enabled, then the remote MiNet sets connected to MBG must also support it. If a MiNet set does not support SRTP, MBG will cause its calls to fail. Notes: MBG supports standard SRTP on both the set side and the switch side (in compliance with RFCs 3711 and 4771). To implement end-to-end security, enable STRP on both the MiVoice Business and MBG. MBG will then facilitate secure communication between remote and local devices. Disable SRTP only when instructed to do so by Mitel Product Support. | Default is Use master setting.
Time zone | Select your time zone from the list or select "----" to have the ICP control the set's time settings. | Default is "----"
Time format | Select 12 hour or 24 hour clock or | Default is Use master setting.
Tone Injection | With this option enabled, a configurable tone will be injected into all calls. See Tone Injection for details. Note: To disable the tone, clear the Enabled option and select Use master. | Default is Use master setting.

Print Page