# Enable Softkeys on the NuPoint UM Server

The following programming tasks are required for the Softkeys feature on the NuPoint UM server:

1. Map new NuPoint Unified Messaging extensions and voice mail ports to the 3300 ICP to allow the ICP software to understand NuPoint softkey interaction. (See Related Topics.)

2. Configure the NuPoint Unified Messaging Server Options and Unified TCP/IP menus to enable network integration and communication.

3. Assign the Softkey Feature Class of Service (FCOS) 10 to all Softkey users' mailboxes. To enable the Softkey feature, include these feature bits in the FCOS for each mailbox:

   - 007 Pause during play and record

   - 050 Play message

   - 053 Keep messages

   - 055 Discard messages

   - 070 User options menu

   - 071 Record or change mailbox name

   - 072 Record or change mailbox greeting

   - 073 Record or change mailbox password

Text Console:

- Mapping NuPoint Extensions and Voice Mail Ports to MiVoice Business software (3300 ICP)

- Configuring Softkeys Integration on the NuPoint UM server