# Category 20: NuPoint Fax Feature Bits

These feature bits control use of the NuPoint Fax optional feature. To use these feature bits, you must have purchased the Fax feature and installed it on the NuPoint Unified Messaging server.

Bit | Description | Required | Incompatible
190 | Receive fax messages | 040 or 041 |
191 | Make fax messages | 020 |
192 | Give fax messages | 024, 190 |
193 | Deliver fax to default number | 070, 190 *110 is required to send a fax to an external machine. It is not required to send internal faxes. |
194 | Deliver fax online | 190 |
195 | *Specify fax delivery number | 070, 190 *110 is required to send a fax to an external machine. It is not required to send internal faxes. |
196 | *Change default fax number | 070, 190, 193 |
197 | Fax-on-Demand for Greeting Only mailbox | 004, 005, 190 |
198 | Receive fax messages only | 190 |
199 | Auto-receipt for successful fax send | 020, 070, 095, 190 |
200 | Personal fax cover page | 190 |
203 | Walkaway fax for callers | 190 |
206 | Discard fax message after delivery |  | 237
207 | Fax Verify (sending system not self) |  | 198
230 | Deny change of fax cover page options | 070, 190 |
235 | Display FROM field on fax cover page | 190 |
236 | Display Promotional Message on fax cover page | 190 |
237 | Automatically delivers fax message to default number | 070, 190 | 206
239 | Retrieve fax on voice recording timeout | 070, 190 |
240 | Receive fax on voice recording timeout | 070, 190 |
247 | Don't play any prompt to fax call placement recipient |  |
256 | Enable fixed greet 'Press1 or wait...' for walkaway fax | 203 |
290 | Enable UM - Web View |  |