# Fax Limits

### Maximum Number of Digits for Telephone Number

Sets the maximum phone number for fax delivery.

Enter: a number from 1 to 25 or '.' to set to default.

Default: 7

### NuPoint Fax Message Count

This is the maximum number of fax messages that can be stored in the mailbox at anytime.

Enter: a number from 0 to 72 or '.' to set to default. (0 = unlimited)

Default: 72

### Pre-greet Silence Interval to Improve Walkaway CNG Detection

This parameter SHOULD be 0!
CNG can be detected during greeting and even recorded. Consequently, an incoming walkaway fax will be taken through the user's greeting or during record if missed during the greet period. This provides an effective dual use mailbox (message or fax). The parameter has been retained as an escape valve in the event extreme circumstances (like noisy lines) affect CNG detection ability.

Enter: '.' to set to default.

Default: 0 (unlimited)

### Fax Delivery Retry Frequency

This is the maximum number of unsuccessful attempts of fax delivery.

Enter: a number from 1 to 255 or '.' to set to default.

Default: 5

### Fax Delivery Retry Interval

This is the number of minutes that the system waits between fax delivery tries.

Enter: a number from 1 to 255 or '.' to set to default.

Default: 5