# MiVoice 5000 or MiVoice MX-ONE SIP Server Configuration

Use these settings only when configuring MiCollab Audio, Web and Video Conferencing with a MiVoice 5000 or MiVoice MX-ONE system. Configure the MiVoice 5000 or MiVoice MX-ONE system first, and then configure the SIP server.

Configure the SIP Server settings in MiCollab Audio, Web and Video Conferencing using the account information from the MiVoice 5000 or MiVoice MX-ONE configuration.

#### To configure the SIP component:

1. From the MiCollab Audio, Web and Video Conferencing main page, click System Options on the navigation pane.

2. In System Options – Platform, select MiVoice 5000 or MiVoice MX-ONE for the system that is connected to MiCollab Audio, Web and Video Conferencing.

3. Click Save, and then click Ok at the prompt to restart the server.

4. Click Configure SIP Server on the navigation pane. The SIP Server Configuration page appears.

5. Enter the following information:

- Extension First: Type the extension number of the first IP device in the hunt group used by the MiCollab Audio, Web and Video Conferencing server to register itself with the PBX.

- Extension Last: Type the extension number of the last IP device in the hunt group used by the MiCollab Audio, Web and Video Conferencing server to register itself with the PBX.

- Extension PIN: This PIN is used for SIP MD5 authentication. If authentication is activated on the MiVoice 5000, this field is mandatory and is equal to the SIP password for subscriber "Extension First" to "Extension Last".

- SIP Domain: This can be the domain name, fully qualified domain name (FQDN), or the IP address of the PBX system used to register the MiCollab Audio, Web and Video Conferencing SIP ports. If you do not know the domain name or FQDN, type the PBX system IP address.

- IP Address: Type the IP address of the PBX system. Alternatively, type the FQDN.
  Note that when typing the FQDN, only the first IP Address value returned by the DNS lookup will be used.

  NOTE: AWV SIP Extension numbers must consist of digits 0 to 9 only. The * and # characters are not supported.

6. Click Save.