# MiVoice 5000 , MiVoice MX-ONE , and MiVoice Office 400 Network Element Field Descriptions

Field | Description | Values
--- | --- | ---
Type | Select network element type required. Mandatory. | MiVoice Business, MiVoice 5000 , MiVoice MX-ONE Service Node, or MiVoice Office 400.
System Name | Enter the unique network element name. For example, "MiV5000_3". Mandatory. This field is read-only for the local MiCollabServer network element. | Enter a unique name of between two and 64 characters in length for the network element. The name can consist of alphanumeric and certain special characters. Spaces are allowed.
IP Address | Enter the IP address of the network element. Mandatory. This field is read-only for the local MiCollab Server network element. Note: For MiVoice MX-ONE deployments, enter the IP address of the MX-ONE Service Node Manager. | Standard IP address notation of four sets of one to three digits separated by periods. For example, 192.168.0.1
Zone | Enter a number to identify the Network Zone. | Number from 1 to 999. Default is blank.
FQDN | Enter a Fully Qualified Domain Name for the network element. | Optional
Outgoing Dialing Prefix | Enter the outgoing dialing prefix to be used by MiCollab Client . | Enter a number up to 32 digits in length. Valid digits are 0 to 9. This field is optional.
Call Forward Destination Directory Number | Enter the NP-UM voice mail number to be used by MiCollab Client. | 10-digit number maximum.
Call Take FAC | This field defines the Feature Access Code that MiCollab Client users dial on a device to which they want to shift an ongoing call from another device and continue the call without interruption. The system copies the code from this field to the PBX Node details page of the MiCollab Client Service. Note: This FAC does not apply to MiVoice Office 250 platform. | MiVoice 5000 default is #70. MiVoice MX-ONE default is *8#. MiVoice Office 400 default is blank. Limit of 16 telephony characters (0-9, *, #)
SIP Conference FAC: | This field defines the Feature Access Code that MiCollab Client users dial to establish a 3-party conference. The system copies the code from this field to the PBX Node details page of the MiCollab Client Service. Note: This FAC does not apply to MiVoice Office 250 or MiVoice Office 400 platforms. A FAC is not used to establish 3-party conferences on these communication platforms. | MiVoice 5000 default is *40. MiVoice MX-ONE default is 3. Limit of 16 telephony characters (0-9, *, #)

Parent topic: Manage Network Elements