# Start/Stop AWV Services

You can start or stop MiCollab Audio, Web and Video Conferencing Service from the Start/Stop AWV tab. This tab displays information including Configuration, ths, mcud, ivrd, cdr_buffer, eocpctl, tnsd, tnsdvr, cpctl, muxerd, awcwss, tnsdvr-monitor status.

Click the Start All button to start all the AWV services. AWV services are started and the screen displays the status information.

Click the Stop All button to stop the running AWV services.

Parent topic: Configuration
↑