# Configure MiVoice Business for MiCollab Audio, Web and Video Conferencing

## Prerequisite in MIVB

- Set Extended Hunt Groups to Yes under License and Option Selection form.

- Select a Class of Service (COS) and SIP Devices Capabilities number from System Properties to be used for MiCollab Audio, Web and Video Conferencing.

- Set Replace System based with Device based In-Call Features to Yes under SIP Devices Capability assignment form.

- Set Suppress Simulated CCM after ISDN Progress to Yes under Class of Service Option (COS) form.

Note: See MiVB System Administration Tool Online Help for more information on the assignment form.

## Configuration on MiVoice Business platform

1. Navigate to Users and devices > Advanced Configuration > IP Telephones > Multiline IP sets, configure the number of virtual extension with device type as Generic SIP Phone.

2. Assign the COS and SIP Devices Capabilities number selected for MiCollab Audio, Web and Video Conferencing to the configured extensions.

3. Under Hunt Groups form, create a hunt group of type Voice. Assign the same COS number selected for MiCollab Audio, Web and Video Conferencing .

4. Add the configured virtual extensions as the members of the hunt group.

## Configuration on MiCollab Server for MiCollab Audio, Web and Video Conferencing

1. From the MiCollab Audio, Web and Video Conferencing main page, click System Options under Configuration.

2. Enter the hunt group number (configured in MiVB) in the Dial-In Phone Number field.

3. Under Platform drop-down list, select MiVoice Business.

4. Click Save, and then click Ok at the prompt.

5. Click Configure SIP Server under Configuration.

6. Enter the first virtual extension DN (created in MiVB) in the Extension First field.

7. Enter the last virtual extension DN (created in MiVB) in the Extension Last field.

8. Enter the SIP Domain name and IP address of the MiVoice Business system used to register the MiCollab Audio, Web and Video Conferencing SIP ports.

9. Enter the SIP Port number of the MiVoice Business system. The port number is 5060.

10. Click Save, and then click Ok at the prompt.

## Additional setting

1. From the MiCollab Audio, Web and Video Conferencing main page, click Web Conferencing Settings under Configuration.

2. Enter the MiCollab Server IP in the Web Conferencing Name field.

3. Click Save, and then click Ok at the prompt.

Note: End-user must verify if the MiCollab Audio, Web and Video Conferencing Client is installed correctly.
Note: Create a new conference from the end-user portal and verify the conference by joining using the access codes.

Additional settings for SIP video support

This setting is enabled to support SIP video option during a MiCollab Audio Web and Video conference. Configure the following on MiVoice Business platform.

1. Navigate to System Properties > SIP Device Capabilities.

2. Under the SDP Option tab, the Allow Device to Use Multiple Active M-Lines option should be set as Yes.