# MiVoice Business SIP Server Configuration

Use these settings only when configuring MiCollab Audio, Web and Video Conferencing with a MiVoice Business system. Configure the MiVoice Business system first. Refer to the MiCollab Installation and Maintenance Guide for more instructions.

After you configure the MiVoice Business system for MiCollab Audio, Web and Video Conferencing, configure SIP Server settings in MiCollab Audio, Web and Video Conferencing using the account information from the MiVoice Business system configuration.

## To configure the SIP component for the MiVoice Business:

1. From the MiCollab Audio, Web and Video Conferencing main page, click System Options on the navigation pane.

2. In System Options – Platform, select MiVoice Business for the system connected to MiCollab Audio, Web and Video Conferencing .

3. Click Save, and then click Ok at the prompt to restart the server.

4. Click Configure SIP Server on the navigation pane. The MiVoice Business SIP Server Configuration page appears.

5. Enter the following information:

   - Extension First: Type the extension number of the first IP device in the hunt group used by the MiCollab Audio, Web and Video Conferencing server to register itself with the MiVoice Business.

   - Extension Last: Type the extension number of the last IP device in the hunt group used by the MiCollab Audio, Web and Video Conferencing server to register itself with the MiVoice Business.

   - SIP Password: Type an alphanumeric User PIN for the MiCollab Audio, Web and Video Conferencing ports on the MiVoice Business. This field is NOT mandatory.

   - SIP Domain: This can be the domain name, fully qualified domain name (FQDN), or the IP address of the Mitel 3300 system used to register the MiCollab Audio, Web and Video Conferencing SIP ports. If you do not know the domain name or FQDN, type the MiVoice Business system IP address.

   - IP Address: Type the IP address of the MiVoice Business system. Alternatively, type the FQDN of the MiVoice Business system.

     Note that when typing the FQDN, only the first IP Address value returned by the DNS lookup will be used.

   - SIP Port: Type the SIP port number of the MiVoice Business system. The port number is typically 5060.

   - Registration Period: Type the number of seconds for the registration period used by the MiCollab Audio, Web and Video Conferencing when it registers itself with the MiVoice Business. Note that this value also controls the registration refresh rate, which is normally half of the Registration Period.

     Note: AWV SIP Extension numbers must consist of digits 0 to 9 only. The * and # characters are not supported.

6. Click Save, and then click Ok at the prompt.

7. Verify the results of the SIP registration process, see Proxy Extension Status.