# Category 11: Make Messages Feature Bits

These feature bits allow a user to record (Make) a message and send it to one or more users. This category also contains two feature bits for timing. Message Addressing, Category 13, controls marking messages “confidential,” and activating return receipts for the messages.

Bit | Description | Required | Incompatible
--- | --- | --- | ---
020 | Make messages (Master) | 040 |
021 | Make and request receipt | 020, 040 |
022 | Make to multiple destinations | 020, 040 |
023 | Make and mark confidential | 020, 040 |
032 | Make to user distribution list | 020, 040, 044 |
034 | Make to master distribution list | 020, 040, 045 |
061 | Wait to record | 022 or 026 |
087 | Make and mark urgent | 020, 040 |
092 | User will be in Dial-by-Name database |  |
096 | Make messages before keep/discard | 020, 040 |
110 | Make/give to telephone number | 020, 024. 040 |
126 | Make/give to mailbox with empty GCOS | 020, 040, 041 |
157 | Repeat message from answering machine | 110 |
158 | Continue sending message | 020 or 024 or 029 |
171 | Cut-through Paging | 070 |
172 | Cut-through Paging and messaging | 070 |
188 | Append # to end of cut-through page number | 070, 171 or 172 |
191 | Make fax messages | 020 |