# Configure a Dialing Plan

1. From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, (R) Reconfigure System.

2. Do one of the following:

   - Select (F) Modify Inactive Configuration if you just made a change through the Offline Menu without activating it

   - Otherwise, select (E) Modify Active Configuration.

3. From the Voice Configuration Menu, select the line group to modify, select (M) Modify Application and then (D) Dialing Plan Menu.

4. For a standard dialing plan, select (D) Dialing Plan. Enter one of the following elements in each of the nine positions as indicated in your NuPoint Voice worksheet, separated by commas:

   Element | Explanation
   --- | ---
   0-11 | Length of the mailbox. Zero means none may start with this number.
   V | Variable number (1 through 11) of digits; server uses timeout to determine end of mailbox number
   M | Analog networking (AMIS) mailboxes leading digit
   A | Dial-by-Name (ASCII) leading digit
   T | Call placement leading digit
   An | Networked mailboxes, n = mailbox number length. NV (variable number length) is acceptable
   Pn | Network mailbox prefix used, n = mailbox length including prefix digit

See Dialing Plan Examples

## Using the Optional Star Prefix Dialing Plan

1. Access the Dialing Plan menu (see steps 1-3 above).

2. To use the Star Prefix dialing plan, select (E) Optional Star Prefix Dplan. For example:

   - If you need a star prefix for Dial By Name, specify the trigger digit:

     Select (E) Dial By Name Dplan Digit and enter the digit that will precede a star to trigger the Dial-by-Name prompt. (For example, to trigger the prompt, "Please enter a mailbox number or press 8 to dial by name." enter "8".)

   - If you need a star prefix for call placement, specify the signal digit: Select (F) Call Placement Msg Delivery Dplan Digit and enter the digit that will precede a star to signal the server that the telephone number following the star is for call placement.

3. Save your entries by exiting to the NuPoint Voice Online Menu. If you chose to modify the Inactive Configuration in step 2, you need to activate the inactive configuration before your changes appear.