# Configure a Speech Recognition Line Group

To add a speech recognition line group to your system configuration:

1. From the navigation tree, click Offline Configuration > Edit Offline Configuration. The Offline Configuration navigation tree opens.

2. When prompted to Duplicate Active Configuration, click Yes.

3. In the navigation tree, click Line Groups and then click Add.

4. Configure the following parameters:

   - Number: Add a number for the line group or click on the Next Available button to add an unused list number.

   - Name: Enter a name for the line group.

   - Application: Select "Speech Recognition" from the list of available applications. The Speech Recognition Application field appears. Note: This line group option is not available if the system is not licensed for speech recognition.

5. On the Speech Recognition tab,

   - Speech Recognition Application: Select the application that corresponds to this line group. This list will be populated according to the speech recognition applications that are currently available on the NuPoint Unified Messaging system. If you select the "VoiceXML Application", then the VoiceXML Start URL field will appear. Enter the URL of the VoiceXML application in this field.

   - Attendant's Extension:Enter the extension number that callers can dial to contact an operator.

6. On the Lines tab, click Add.

7. Configure the following additional parameters:

   - Line Triplet: Enter a line number for the line group or click on the Next Available button to add an unused line number.

   - Number of Lines: Enter the number of lines in this line group.

   - PBX: Select the PBX to use for this line group.

   - Mapping: In a multi-node system, enter the module number, line card number, or port designator to add to the line group.

   Note: Support for multiple-module servers (e.g. NPM UM 640) was discontinued with NuPoint Release 6.0.

8. Click Add to save the configuration data.

9. Click Save to add the new line group to the list of existing line groups. A confirmation message regarding the configuration changes appears.

10. In the navigation tree, select Commit Changes and Exit. Confirm the commit. Your changes are now saved to the duplicate (inactive) configuration. Configuration changes will not take effect until you have activated the inactive configuration.