# Network Usage Statistics Report

## Overview

The Network Usage Report gives 15-minute "snapshots" of network message activity for a specified reporting period. This period can be any hour or range of hours from the current day or the previous six days. A sample of a Network Usage report is shown here:

                  >>>
    Mitel Corporation<<<
NETWORK USAGE 15min REPORT Mon Nov 16, 20XX 10:53 am 11/16/XX 8hr-9hr --- minutes interval --- MESSAGE DAY=01 HOUR=08 00-14 15-29 30-44 45-59 AVERAGE BATCH IN QUEUE 0 0 0 0 0 URG IN QUEUE 0 0 0 0 0 BATCH MAX LENGTH 0 0 0 0 - URG MAX LENGTH 0 0 0 0 - BATCH LATENCY H:M:S 0:00:00 0:00:00 0:00:00 0:00:00 - URG LATENCY 0:00:00 0:00:00 0:00:00 0:00:00 - BATCH DELIVERED 0 0 0 0 0 URG DELIVERED 0 0 0 0 0 TOTAL UNDELIVERED 0 0 0 0 0 BATCH RECEIVED 0 0 0 0 0 URG RECEIVED 0 0 0 0 0 UNDLV RMT MBOX 0 0 0 0 0 UNDLV NETQ FULL 0 0 0 0 0 TOTAL FRAME TX 0 0 0 0 0 TOTAL FRAME RX 0 0 0 0 0 UNDLV NWK 0 0 0 0 0 NETWORK UNDELIVERED 0 0 0 0 0 RECIPIENT UNDELIVERED 0 0 0 0 0 MBOX NO STAT 0 0 0 0 0 MBOX IS NIB 0 0 0 0 0 MBOX IS VM 0 0 0 0 0 MBOX FULL 0 0 0 0 0 MBOX NOACCT 0 0 0 0 0 WRONG MBOX FCOS 0 0 0 0 0 WRONG MBOX GCOS 0 0 0 0 0 WRONG MBOX NCOS 0 0 0 0 0 NET MSG FAIL 0 0 0 0 0 NET NODE FAIL 0 0 0 0 0 MSG IS MSG 0 0 0 0 0 MSG IS NAME 0 0 0 0 0 MSG IS GREET 0 0 0 0 0 MSG IS RCPT 0 0 0 0 0 FORCE RCPT 0 0 0 0 0 MSG >=5MIN 0 0 0 0 0 MSG >=1MIN 0 0 0 0 0 MSG LT 1MIN 0 0 0 0 0 MSG HAS FAX 0 0 0 0 0 NIB ACK RCPT 0 0 0 0 0 NIB RECIP FULL 0 0 0 0 0 NIB RECIP NUSR 0 0 0 0 0 NIB NWK PROB 0 0 0 0 0 NIB CNT ERROR 0 0 0 0 0 NIB WRONG FLAG 0 0 0 0 0 NIB OUT OF RANGE 0 0 0 0 0 NIB NO COPY LST 0 0 0 0 0 NIB WRONG CRTIME 0 0 0 0 0 NIB WRONG INDX 0 0 0 0 0

## Reading the Standard Network Usage Report

In the sample report, the heading shows the node name, the report name, the date, and the time that the report was run.

The first line shows the date and time interval when the data were gathered.

HYPHEN (-) (In any column) indicates that the system was not processing messages during the report period (for example, during a power failure or when the system was taken offline for maintenance). A 0 (zero) in any column means the system was operable, but there was no activity.

MESSAGE DAY = 01, HOUR = 08 Indicates that the data displayed immediately below were gathered on Monday, during the hour between 8 a.m. and 9 a.m. Entry 00-14 indicates that data in the column were gathered during the first 15-minutes of the hour; 15-29 refers to the second 15-minutes of the hour; 30-44 refers to the third 15-minutes of the hour; 45-59 refers to the last 15-minutes of the hour.

AVERAGE The average value of the four 15-minute samples. If a hyphen appears in place of a numerical value, it means that the data have not been gathered.

EXAMPLE:If the report is run at 3:30 p.m., and the report interval is for hours 12-15 (noon

to 3 p.m.) of the same day, the entries for hour 15 (3 p.m. to 4 p.m.) will be hyphens.

BATCH IN QUEUE The total number of batch (non-urgent) messages and receipt updates present in the network queue during the time period.

URG IN QUEUE The total number of urgent messages in the network queue during the time period.

BATCH MAX LENGTH The total number of minutes of recorded speech in the network batch queue during the time period.

URG MAX LENGTH The total number of minutes of recorded speech in the urgent network queue during the time period.

BATCH LATENCY The maximum number of seconds that a message remained in the batch network queue during the time period.

URG LATENCY The maximum number of seconds that a message remained in the urgent network queue during the time period.

BATCH DELIVERED The total number of batch messages delivered to their destination nodes during the time period. (Receipt updates do not count.)

URG DELIVERED The total number of urgent messages delivered to their destination nodes during the time period.

TOTAL UNDELIVERED The total number of messages (batch and urgent) rejected by their destination nodes during the time period. (Receipt updates do not count.)

## The Network Usage Summary Report

The Network Usage Summary Report gives peak (maximum) and total statistics for network message activity during a specified reporting period.

PEAKS Statistics for maximum activity during the reporting period. Although separate statistics are kept for batch and urgent message queues, these statistics are not broken down by destination node. In other words, urgent queue statistics refer to urgent messages accumulated for every node on the network.

## Run the Network Usage Report

1. From the Main Menu, select (R) Reports, (S) Statistics, and then (N) Network Statistics.

2. In the Speech Blocks Usage menu:

   - select (A) Beginning Hour and enter the first hour of the time period to report (0 = midnight; 12 = noon. Default is 8)

   - select (B) Ending Hour and enter the last hour of the time period to report. (Default is 17.)

   - select (C) Beginning Day and enter the first day of the week to report (Sun-Sat = 0-6. Default is Mon - Fri.)

   - select (D) Ending Day and enter the last day of the week to report

   - (optional) select (E) Summary = and choose N for detailed report or Y for a summary report. (Default is N.)

   - select (R) Run report

3. Select an output routing for the report:

   - C to send the report to the console without pausing

   - F to send the report to a file on the server

The standard Network Statistics Report displays data for each hour of the chosen interval, in 15-minute increments. The summary report shows a single value for each hour.

Parent topic: Procedures (Text Console)