# LCOS Parameters and Default Values (Web Console)

LCOS 1 is pre-configured; it contains the default values for all parameters. All mailboxes are assigned LCOS 1 by default, unless otherwise configured by the system administrator.

## Limits Values - Web Console Layout

General Limits | Unit | Default | Minimum | Maximum | Notes
--- | --- | --- | --- | --- | ---
Greeting length | Minutes | 2 | 0 | 60 | Sets the maximum time for recording a personal greeting. When the user reaches this limit or the server detects silence, the server stops recording and announces that the recording is complete. If no limit is set, the limit is the available storage capacity. Can also be disabled.
User name length | Seconds | 2 | 0 | 240 | Sets the maximum time for recording the mailbox name. When the user reaches this limit or the server detects silence, the server stops recording and announces that the recording is complete. If no limit is set, the limit is the available storage capacity. This name is announced when the user makes or gives a message; also used by NP Receptionist.
Message count |  | 200 | 0 | 200 | Sets the maximum number of messages in a single mailbox. When the user's mailbox is 80% full, the system will warn the user to "delete any unnecessary messages" as follows: An audible prompt will be played when the user logs in to his or her mailbox. An email message will be sent to the user's Standard or Advanced UM address (programmed in the mailbox parameters). The email message re-issued on a daily basis and includes a link to the Web View application, where the user can log in and begin deleting or archiving messages. When the user's mailbox is 100% full, callers and other users cannot leave messages. Note: When a user answers or forwards a message, each attachment to the original counts as a single message. For example, if the limit is 10 and one message has 9 attachments, it fills the mailbox. For systems that upgrade to release 4.1 or later from a pre-4.1 release, this LCOS parameter carries forward a default of 73 messages.
User message length | Minutes | 5 | 0 | 60 | Sets the maximum time, in minutes, that another user can make, give or answer a message for this mailbox. When the user reaches this limit or the server detects silence, the server stops recording and announces that the recording is complete.
Caller message length | Minutes | 5 | 0 | 60 | Sets the maximum time, in minutes, that a caller can leave a message for this mailbox. When the caller reaches this limit or the server detects silence, the server stops recording and announces that the recording is complete.
Maximum login time | Minutes | 0 (unlimited) | 0 | 50 | Sets how long, in minutes, a user can remain logged in to the mailbox in a single session. At the end of this time, the server automatically logs the user out.
Maximum attachments per page |  | 199 | 0 | 199 | Limits the number of messages that the user can attach when making or giving a message.
Future delivery message count |  | 99 | 1 | 99 | Sets the maximum number of messages that can be stored in a mailbox’s future delivery queue. Enter 0 to disable.
Future delivery maximum days | Days | 60 | 1 | 365 | Sets the maximum delay, in days, to deliver a message in the future. Enter 0 to disable.
Minimum message length | Seconds | 0 (unlimited) | 0 | 5 | Sets the shortest time for a message to be considered valid. Shorter messages are not delivered.
Minimum recipients count |  | 65535 | 0 | 65535 | Sets the minimum number of recipients needed to activate a receipt summary. The system then plays receipts in this order: for undelivered messages, unplayed messages, then played messages. 0 = the maximum (65535)
Maximum recipients count |  | 65535 | 0 | 65535 | Sets the total number of possible recipients of a message in any combination of mailboxes, distribution lists, and nested distribution lists. If the number of recipients exceeds this limit (n), the system sends the message to only the first (n) recipients. 0 = the maximum (65535)
Passcode Expiry Period | Days | 0 | 0 | 365 | Enter 0 to disable.
Wake UP Limits | Unit | Default | Minimum | Maximum | Notes
Phone length | Number of Digits | 11 | 1 | 24 | Sets the maximum number of digits a user can enter for a wakeup call phone number.
Maximum days | Days | 0 (unlimited) | 0 (unlimited) | 365 | Limits the time in the future that a user can schedule a wakeup call.
Billing Limits | Unit | Default | Minimum | Maximum | Notes
Maximum pages per billing |  | 0 (unlimited) | 0 (unlimited) | 999 | Sets the maximum number of times a user can be paged during one billing cycle.
Maximum wake-up per billing |  | 5 | 0 (unlimited) | 999 | Sets the maximum number of wakeup calls a user can schedule during one billing cycle.
Minimum billed number length | Number of Digits | 0 | 0 | 25 | Sets the minimum number of digits in a dial string to activate billing for outdials.
Call Placement Limits | Unit | Default | Minimum | Maximum | Notes
RNA retry limit | Retries | 5 | 1 | 255 | Sets how many times the server tries to deliver a call placement message after a Ring No Answer call.
RNA retry interval | Minutes | 5 | 1 | 255 | Sets how long the server waits between tries to deliver a call placement message after a Ring No Answer call.
Busy retry limit | Retries | 5 | 1 | 255 | Sets how many times the server tries to deliver a call placement message after a Busy call.
Busy retry interval | Minutes | 5 | 1 | 255 | Sets how long the server waits between tries to deliver a call placement message after a Busy call.
Message phone length | Number of Digits | 11 | 1 | 25 | Sets the maximum number of digits a user can enter for a call placement phone number.
Recipient count |  | 190 | 0 | 190 | Sets maximum number telephone numbers you can enter at any one time, for a single message. This includes both call placement, and AMIS messages
Maximum message length | Minutes | 5 | 0 (unlimited) | 60 | Sets how long a message can be for a call placement phone number.
Distribution List Limits | Unit | Default | Minimum | Maximum | Notes
Maximum members per list |  | 200 | 0 (unlimited) | 65535 | Sets the total number of possible recipients of a message in any combination of mailboxes, distribution lists, and nested distribution lists. If the number of recipients exceeds this limit (n), the system sends the message to only the first (n) recipients.
Maximum number of lists |  | 99 | 0 (unlimited) | 99 | Sets the maximum number of distribution lists allowed in a mailbox.
Fax Limits | Unit | Default | Minimum | Maximum | Notes
Maximum number of digits | Digits | 11 | 1 | 25 | Sets the maximum phone number for fax delivery.
Fax message count |  | 199 | 0 | 199 | This is the maximum number of fax messages that can be stored in the mailbox at anytime.
CNG tone detection length | Seconds | 0 (unlimited) |  |  | This parameter SHOULD be 0! Starting with the NuPoint Messaging architecture, CNG can be detected during greet and even record. Consequently, an incoming walkaway fax will be taken through the user's greet or during record if missed during the greet period. This provides an effective dual use mailbox (message or fax). The parameter has been retained as an escape valve in the event extreme circumstances (like noisy lines) affect the CNG detection ability.
Fax delivery retry limit | Retries | 5 | 1 | 255 | This is the maximum number of unsuccessful attempts of fax delivery.
Fax delivery retry interval | Minutes | 5 | 1 | 255 | This is the number of minutes that the system waits between fax delivery tries.
ISO User Interface Limits | Unit | Default | Minimum | Maximum | Notes
Maximum family members or guests |  | 0 (unlimited) |  |  | Not used.
Reminder calls maximum days | Days | 0 (unlimited) |  |  |
Maximum reminder calls per billing |  | 0 (unlimited) |  |  |
Maximum destinations per reminder |  | 0 (unlimited) |  |  |
Language | Unit | Default | Minimum | Maximum | Notes
Language |  | Default | N/A | N/A | Only installed languages can be assigned. Select a language from the drop-down list.
Message Age Limits | Unit | Default | Minimum | Maximum | Notes
Played messages retention | Hours | 672 | 1 | 8760 | Sets how long a played message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Unplayed messages retention | Hours | 336 | 1 | 8760 | Sets how long an unplayed message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Urgent messages retention | Hours | 336 | 1 | 8760 | Sets how long a played or unplayed urgent message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Cut-thru paging receipt retention | Hours | 672 | 1 | 8760 | Sets how long a receipt for a cut-through paging message can remain in a mailbox before it is deleted by automatic purging. For more information, see the Cut-Through Paging. 0 means unlimited.
Receipt retention | Hours | 672 | 1 | 8760 | Sets how long a receipt for a message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Played fax retention | Hours | 672 | 1 | 8760 | Sets how long a played Fax message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Unplayed fax retention | Hours | 336 | 1 | 8760 | Sets how long an unplayed Fax message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Urgent fax retention | Hours | 336 | 1 | 8760 | Sets how long a played or unplayed urgent Fax message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Fax receipt retention | Hours | 672 | 1 | 8760 | Sets how long a receipt for a Fax message can remain in a mailbox before it is deleted by automatic purging. 0 means unlimited.
Absolute message retention | Hours | 0 | 0 | 8760 | Sets how long a message stays in the mailbox if the user does not delete it. Note: If you set this to less than the values for the Played and Unplayed message retention parameters, it overrides them. If this is set to 0 (the default), it is ignored. 0 means unlimited.
MWI Limits | Unit | Default | Minimum | Maximum | Notes
Paging Phone Length | Digits | 11 | 1 | 24 | Sets the maximum number of digits a user can enter for a pager phone number.
Message delivery phone length | Digits | 11 | 1 | 24 | Sets the maximum number of digits a user can enter to for a message delivery phone number.
MWI message length | Minutes | 0 (unlimited) | 0 | 5 | Sets the shortest time for a message that will activate message waiting or paging for the mailbox.
Network Limits | Unit | Default | Minimum | Maximum | Notes
Network queue message count |  | 99 | 1 | 99 | Limits how many messages a user can make or give for remote delivery. For more information, see NP Net.
Maximum attachment per network message |  | 199 | 1 | 199 | Limits the number of messages that the user can attach when making or giving a message in a network environment. For more information, see the NP Net and VPIM optional features.
Maximum hours to wait for reply from NIB | Hours | 0 |  |  | Not used.
Outdial Applications Limits | Unit | Default | Minimum | Maximum | Notes
Minimum billed number length | Digits | 0 | 0 | 25 | Sets the minimum number of digits in a dial string to activate billing for outdial.
Call Director Template | Unit | Default | Minimum | Maximum | Notes
Template |  | No Template | N/A | N/A | Only existing templates can be assigned. Select a template from the drop-down list.
Unified Messaging Limits | Unit | Default | Minimum | Maximum |
Unified Messaging Limits |  | Yes |  |  | For Standard Unified Messaging users. By default, the system forwards voice mail messages to email clients as audio attachments, links to audio files, links to messages in Web View, or text notifications. To save hard drive space you can limit notifications to text format only. Setting unified messaging limits (selecting "No" for "Allow All SMTP Delivery Options" overrides all FCOS settings that relate to call forwarding.

Parent topic: Procedures (Web Console)