# Modify the Node Number for a Prefix

Use this procedure to change the node number and number of digits to absorb associated with a prefix in the Digits Translation Table.

1. From the Main Menu, select (S) System Maintenance, (W) Network Menu, (M) Network Maintenance, and then (D) Digit Translation Menu.

2. Select (M) Modify the node number for a prefix and enter a valid prefix number or hyphen-separated range of numbers.

3. At the New node number: prompt, enter a valid node number.

4. At the Absorb cnt: prompt, enter the number of digits (0-12) to absorb. The system displays the prefix to modify and prompts you to confirm.

5. Press Y to confirm modification or N to leave unchanged.

Parent topic: Digits Translation Table Tasks