# Configuring the MCD Softkeys Integration on the NuPoint UM Server

Perform the following steps to configure softkey integration in the MCD Note: This release marks the introduction of separate brands for the Mitel range of hardware and software-only solutions for the IP communications market. Mitel Communications Director (MCD) is the brand name of the call-processing software that runs on hardware platforms such as the 3300 ICP. The 3300 ICP name continues as the brand for Mitel hardware platforms that run MCD. 3300 ICP Release 9.0 is the last software release under the old branding scheme; its successor is MCD 4.0. software on the 3300 ICP:

1. From the Main menu, select (S) System Maintenance, (R) Reconfiguration, (R) Reconfigure System, and then (G) Offline Menu. If you want to duplicate the configuration, select (B) Duplicate Active Configuration. All programming procedures from this point on will affect only the duplicate configuration and will only take effect after the configuration is activated.

2. Select (I) Server Options Configuration and then select (C) Configure 3300 ICP integration.

3. Map the 3300 ICP integration by entering the following configuration information. Note that each of the following entries must match the information entered in the 3300 ICP System Options form.

   - (N) The name of 3300 ICP server to be configured for softkey integration with the NuPoint Unified Messaging server, for example, [pbx3].

   - (I) The 3300 IP address to which you are mapping, for example [10.37.237.150]

   - (S) The set registration code that matches with the code entered in the System Options form on the 3300 ICP. (Default is ***.)

   - (R) The set replacement code. (Default is ###.)

4. Exit to the OFFLINE MENU prompt.

5. Select (U) Unified TCP/IP Menu and then select (M) Configure a Module to access the Ethernet Configuration Menu.

6. In the Ethernet menu, select and enter the required configuration parameters as shown here:

   - (C) Current Module Number = [1]

   - (D) Enable or Disable Current Card = [Enable]

   - (E) Ethernet Card Configuration = [1]

   - (G) Optional Arguments for the card driver = [-y20]

   - (H) Node Name = [node1]

   - (I) Node IP Address = [10.37.237.222]

   - (J) DNS IP Address = []

   - (M) Subnet Mask = [255.255.255.0]

   - (N) Network Number = [1]

   - (O) Broadcast Address = []

   - (P) Operation Mode (Primary/Secondary) = [Primary]

   - (R) Driver Id = [2]

   - (S) Current Card Slot Number = [1]

   - (T) Gateway IP Address = [10.37.237.1]

   - (U) TELNET Configuration (Enable/Disable) = [Enabled]

   - (V) Smart Host Domain Name = [dc3.dcexg3.saelab.com]

7. Exit from this menu, and return to the Offline Menu to save your configuration settings. If you chose to duplicate the active configuration in step 1, you need to activate the inactive configuration before your changes will take effect.