# Category 1: Greeting Feature Bits

These feature bits control events that occur during or immediately after the mailbox greeting is played.

To allow the mailbox user to record the mailbox greeting, the FCOS must also contain the following feature bits:

- 070 (User Options Menu)

- 072 (Record or change mailbox greeting)

Bit | Description | Required | Incompatible
--- | --- | --- | ---
060 | Ignore DTMF’s during greeting |  | 164
062 | Hang up immediately after greeting |  | 063, 064, 065
063 | Call mailbox attendant after greeting |  | 062, 064
064 | Call mailbox user extension after greeting |  | 062, 063
065 | Play system time after greeting |  |
161 | Conditional greetings | 070 |
162 | General greetings | 070 |
164 | Skip/pause greeting in greeting only mailbox | 062 | 060
224 | *Auto transfer to task before greeting | 170 |
297 | Enable Extended Absence Greeting | 161 |
298 | Disable Message Delivery when Extended Absence Greeting is Enabled | 297 | 133

Parent topic: Feature Bits by Category