# Configure WebRTC Settings

Complete the following procedures to enable MBG to support the WebRTC application.

Configure WebRTC Settings

To configure WebRTC settings on MBG:

Note: Since these values are included in the SDK, program them before you download the SDK.

1. On the MBG main page, click the Teleworking tab and click WebRTC.
2. Enter or edit the options as required and click Save:

   Field | Description | Notes
   Hosting Mode | Select the location of the WebRTC web site: Host WebRTC client locally: The WebRTC client is hosted on the MBG web server. Host WebRTC on separate server: The WebRTC client is hosted on a standalone web server, either the MiCollab web server or, if your implementation includes a MiVoice 5000 ICP, your enterprise web server. | If you select Host WebRTC client locally, configuration is complete when you save the WebRTC settings. Users may then initiate a call by entering the following addresses in a web browser: Anonymous call mode https://<MBG-FQDN>/webrtc/call.php?to=<CalledNumber | SipUri> Subscriber call mode https://<MBG-FQDN>/webrtc/index.php If you select Host WebRTC client on separate server and choose to employ the WebRTC client that is pre-installed on the MiCollab web server, configuration is complete when you save the WebRTC settings. Users may then initiate a call by entering the following addresses in their MiCollab Web Client: Subscriber call mode <https://<MiCollab-server_FQDN>/ucs/micollabwebrtc> If you select Host WebRTC client on separate server and choose to host the WebRTC client on your enterprise web server, after saving the WebRTC settings, you must download the Software Development Kit (SDK), modify the files contained in the kit to suit your requirements, and then upload the files to your enterprise web server. For details, see Configure Web Server for WebRTC. Users may then initiate a call by entering the following addresses in a web browser: Anonymous call mode https://<standalone-web-server-FQDN>/webrtc/call.php?to=<CalledNumber | SipUri> Subscriber call mode https://<standalone-web-server-FQDN>/webrtc/index.php Note: To host the WebRTC client on your enterprise web server, your implementation must include the MiVoice 5000; other ICPs are not supported.
   Enabled | Displays the status of the WebRTC service. |
   Mode | Select the call mode(s) that users can employ to initiate calls from their web browsers: Anonymous: Users can initiate anonymous click-to-call sessions from a browser to the call controller. To access this service, users are required to provide minimal credentials (name and CAPTCHA entry). MBG then directs them to an internal service that has been configured on the Anonymous WebRTC ICP. Subscriber: Users can access the company directory and place calls from a browser using a SIP web phone. To access this service, users are required to provide their MBG login credentials (set-site username and password). MBG then registers them with an ICP that has been configured on the ICPs screen. Anonymous and Subscriber: Users can initiate both anonymous and subscriber calls. | A CAPTCHA is a type of challenge-response test used to determine whether or not the user is human.
   Webserver shared secret | Enter the password shared between MBG and the web server. | This value must be set even when the MBG system is configured to function as a web server.
   Anonymous WebRTC ICP | Select the ICP to which WebRTC clients will connect. The following ICP types are supported: MiVoice Business MiVoice 5000 | Only one ICP can be selected for each MBG that is configured to support WebRTC Anonymous calls. Multiple ICPs are not supported. Note: Multiple ICPs are supported for WebRTC Subscriber calls. When a user logs in, he or she provides their MBG login credentials (set-site username and password); MBG then registers the user with one of the ICPs configured on the ICPs screen.
   WebRTC protocol security mode | This field controls encryption for WebRTC communications. Two options are available: Public only: Encryption is enabled for WebRTC communications on the public interface of MBG (the Internet) but not the private interface. Public and Private: Encryption is enabled for WebRTC communications on both the public and private interfaces of MBG. Currently, this mode is available only with MiVoice 5000, not with MiVoice Business. For encryption to work properly on the public interface of the WebRTC server, you must configure the system with a third-party web certificate as follows: Add the 3rd-party Web Server Certificate. Enable WebRTC feature. | The secured protocols usedon the public interface of MBG are: HTTPS (for web pages and services). SIP over WSS for signaling. DTLS-SRTP for media. The secured protocols used on the private interface of MBG are: SRTP over UDP for media. Note: WebRTC restarts automatically after the certificate is installed to ensure all components and services that require the certificate are informed of the certificate's presence.
   WebRTC whitelist/blacklist mode | This field controls the operation of the whitelist/blacklist security feature that can be enabled on the WebRTC application. The whitelist consists of "trusted addresses" belonging to ICPs that are configured on MBG. The blacklist consists of "untrusted addresses" belonging to endpoints that are suspected of malicious behavior such as brute force attacks. Neither: The feature is disabled. All addresses are allowed. Whitelist and Blacklist: Addresses on the whitelist (trusted ICPs) are allowed. Addresses on the blacklist (untrusted endpoints) are blocked. | An address will be dropped from the blacklist after five hours, provided that it does not engage in suspicious behavior during that time.
   Video enabled | Select to enable video in addition to audio. Clear to enable audio only. To take advantage of this feature, both SIP endpoints must support the VP8 codec. Otherwise, transcoding must be enabled. | When this field is enabled, users will see a video panel on the call web site. If this field is disabled, the video panel will not appear.
   Transcoding enabled | Select to enable transcoding to/from the codecs supported by WebRTC web clients (VP8) and Mitel devices (G.711 and H.264). | Transcoding video can be CPU intensive. To prevent your system from experiencing issues, you may need to instruct your users to limit the number of video calls that they place at any one time. If your implementation includes the Mitel MiVoice Video Phone (UC360), enable Transcoding to support video calls.
   LDAP server | If you are using Subscriber call mode in conjunction with the MiVoice 5000, and you wish to look up/retrieve user information from an LDAP database such as Active Directory, enter the address of the LDAP server. For example, to use the LDAP database included with the MiVoice 5000, enter the address of the MiVoice 5000. |
   LDAP DN | Enter the LDAP Distinguished Name. |
   LDAP login | Enter the LDAP login ID. |
   LDAP password | Enter the LDAP login password. |
   Pictures server URL | If you are using Subscriber call mode and wish to retrieve user images from a media server, enter the URL of the server. For example, to use the media server included with the MiVoice 5000, enter https://hostname/photos/local/ as the URL. | The image files require the following format: <number>.png Where <number> is each user's telephone number.
   Voicemail digits | Enter the telephone number required to access the voicemail system. Typically, this is a hunt group number. |

WebRTC Port Ranges

If your solution is in a container, WebRTC Port Ranges are auto-configured at deployment, and cannot be modified.

Parent topic: WebRTC Implementation