# Configuration Overview

The MBG interface displays the following configuration tabs and sub-menus:

Tab | Sub-menu | Tasks
--- | --- | ---
System | Dashboard | view configure status and system information, plus enable/disable MBG service
Metrics | view statistical information like Connections, Active Calls, and Calls per Hour
Connectors | view detailed status of all connectors
Settings | view/edit advanced system settings (service parameters, global settings, MiNet options, SIP options, logging configuration)
Trust Store | view the list of certificates in the configurable trust store
Bulk provisioning | manage device data
Network | Profiles | pre-configured profiles to set up your network configuration
ICPs | set up the ICP or system that interacts with MBG
Port ranges | pre-configured range of ports available for use by MiNET and SIP calls
IP blocking | view/configure network activities in real-time and block or allow connections between MBG and specific network blocks in CIDR format
MiNet fallback addresses | configure manual fallback IP address (for device reboot)
Teleworking | Status | view MiNet and SIP profiles and devices
WebRTC status | view list of WebRTC registered clients and calls in progress
MiNet | add/edit MiNet phones and devices that connect to the server
SIP | add/edit SIP phones and devices that connect to the server
WebRTC | configure the WebRTC gateway to support browser-based voice and video calls
Application integration | enable for Mitel Performance Analytics (MPA). For steps to create MPA Probe refer to MiCloud Flex on GCP Deployment Guide.
SIP trunking | Status | view SIP trunk status
Configuration | view/configure SIP trunks
Adaptation | configure SIP adaptation pipelines, and their plugins
Call recording | Status | view status of all registered call recording equipment
Configuration | configure call recording
Troubleshooting | Diagnostics | Fetch logs for product support: Downloads MBG log files as a single compressed archive. Connectivity Tests: Checks connectivity to ICPs for MiNET, SIP, and TFTP services based on the configured type; SIP trunking endpoints; and application servers such as MiCollab and MiContact Center. If these are configured with a fully qualified domain name (FQDN), a DNS resolution test is also run. Packet Trace: Capture a log of traffic passing over the network. Teleworker Network Analyzer: Tests voice quality and remote IP Phone connectivity to the MBG server.
Logging | Primary Service: Controls logging for SIP and MiNet devices, SIP trunks, call recording, and clustering. WebRTC Service: Controls logging of WebRTC user registrations and calls.
Alarms | set the severity level for individual events. set the thresholds for SNMP traps
Overrides | view list of configuration overrides

## Configuration Steps

The following services are pre-configured during initial deployment of the solution:

- MiNet support and MiNet options for local streaming and ping before redirect
- SIP support and SIP options, including required allowed_uri
- ICPs
- Network Profile
- Port ranges
- Clustering
- Application Integration Voice Quality
- SIP trunking (using MiConfig Wizard)
- WebRTC support

Optionally, the following can be configured:

- Additional SIP Trunks
- Call Recording
- SIP options Set-side and ICP-side RTP security

Parent topic: General