# Configure Call Recording

Parent topic: Call Recording Service

## Configure SRC

To configure MBG for a call recording deployment with Mitel Secure Recording Connector, follow these steps:

1. Review the call recording port ranges.
2. Enable the service.
3. On the MBG main page, click Call recording > Configuration. In the Secure Recording Connector frame, select the Enabled check box.
4. Select the secure connection mode matching your CRE implementation:
   1. MTLS (Mutual TLS): Select this mode if your CRE requires a certificate to connect and Enroll the CRE.
   2. PSK (Preshared key): Select this mode and configure a matching password to the one configured on your CRE.
   Note: For direct call recording, select Tone Injectionoptions (optional).
5. Click Save.

## Configure SIPREC

To add a SIP Recording Server to MBG:

1. On the main page of each MBG in a cluster, click the Call recording tab and then click Configuration.
2. Click in the SIPREC server section.
3. Update the SIPREC Server Options as required and then click Save.

   Field | Description | Notes
   --- | --- | ---
   Enabled | Select this check box to enable the SIPREC server.Clear the check box to disable. |
   Host | Enter the IP address or hostname of the SIPREC server followed by the port number. For example, 1.2.3.4:5060 srs.mycompany.com:5061 | Default SIP port is 5060 for TCP and 5061 for TLS.Your SIPREC server may use a non-default SIP port.
   Transport | Use the drop-down to select the transport to connect to the SIPREC server: TCP TLS | Default is TCP. The selected transport must also be enabled under SIP settings.
   Contact | Use the drop-down to select which IP address MBG should include in the SIP message with the SIPREC server. | Default is the LAN IP of MBG.
   Media | Use the drop-down to select the encryption parameters of the recorded audio sent to the SIPREC server: RTP "AES_CM_128_HMAC_SHA1_32 "AES_CM_128_HMAC_SHA1_80 | Default is RTP.
   Preserve TO header | Select this check box to have MBG use the recording device extension in the SIP To header and in the SIPREC body. | By default, MBG uses a username of siprec in the SIP To header of all messages sent to the SIPREC server.

### Edit SIPREC server

To edit a SIPREC server:

1. On the MBG main page, click the Call recording tab and then click Configuration.
2. In the SIPREC servers listing, locate the server you want edit and click .
3. Edit the information as required.
4. Click Save.

### Delete SIPREC server

To delete a SIPREC server:

1. On the MBG main page, click the Call recording tab and then click Configuration.
2. In the SIPREC servers listing, locate the server you want delete and click .