# Voice Quality Statistics Integration

Use this procedure to configure settings for integration with a third-party fault and performance management application such as the Mitel Performance Analytics (MPA).

Once the connection has been configured, MiVoice Border Gateway will forward its voice quality statistics to the remote application in the form of JSON-based RTCP data or through SIP PUBLISH messages to a configured server (such as a Voice Quality collector). The remote application will capture and interpret the data, and then graph it for use by system administrators.

To configure Voice Quality Statistics Integration settings:

1. On the MBG main page, click the Teleworking tab and click Application integration.

2. Click to add a record.

3. In the Voice Quality Statistics Integration frame, enter or edit the options as required and then click Save:

Field | Description
Format | Select the format for the data: JSON: MBG generates JSON RTCP data for MiNet Teleworker set calls and SIP Trunk calls that flow through MBG. MBG sends the JSON RTCP data to the Voice Quality Collector. SIP PUBLISH: MBG forwards RTCP Summary reports it receives (for example, MiCollab Client Softphone in Teleworker mode) on its SIP Signaling connections to the RFC-6035 compliant Voice Quality collector (such as, the MPA Probe).
Address | Enter the IP address of the remote fault and performance monitoring application. MBG will send voice quality statistical data to this address.
UDP Port | Enter the UDP port number of the remote fault and performance monitoring application. MBG will send voice quality statistical data to this port. Note: Ensure that the UDP ports are the same as those configured in the Voice Quality Reporting app.

Parent topic: Application Integration
↑