# Configure Call Recording

Parent topic: Call Recording Service

## Configure SRC

To configure MBG for a call recording deployment with Mitel Secure Recording Connector, follow these steps:

1. Enroll the CRE
2. Review the call recording port ranges.
3. Enable the service. On the MBG main page, click Call recording > Configuration. In the Secure Recording Connector frame, select the Enabled check box.
   Note: For direct call recording, select Tone Injection options (optional).
4. Select the secure connection mode matching your CRE implementation:
   1. MTLS (Mutual TLS): Select this mode if your CRE requires a certificate to connect and Enroll the CRE.
   2. PSK (Preshared key): Select this mode and configure a matching password to the one configured on your CRE.
5. Click Save.

For indirect call recording:

1. On the MBG main page, click the Network tab and click ICPs.
2. Click to add a new ICP or to edit an existing ICP.
3. Select indirect call recording capable and other ICP settings, and then click Save.

For direct call recording:

1. Configure your MiNet devices, SIP devices, or SIP trunk.
2. Restrict codecs for MiNET and SIP if required by your CRE.

To review the list of connected CREs and number of calls that are being recorded, see Call recording status.

To configure MBG for a call recording deployment with Mitel Secure Recording Connector, follow these steps:

1. Review the call recording port ranges.
2. Enable the service.
3. On the MBG main page, click Call recording > Configuration. In the Secure Recording Connector frame, select the Enabled check box.
4. Select the secure connection mode matching your CRE implementation:
   1. MTLS (Mutual TLS): Select this mode if your CRE requires a certificate to connect and Enroll the CRE.
   2. PSK (Preshared key): Select this mode and configure a matching password to the one configured on your CRE.
   Note: For direct call recording, select Tone Injectionoptions (optional).
5. Click Save.

↑