# Voice Quality Statistics Integration

Use this procedure to configure settings for integration with a third-party fault and performance management application such as the Mitel Performance Analytics (MPA).

Once the connection has been configured, MiVoice Border Gateway will forward its voice quality statistics to the remote application in the form of JSON-based RTCP data. The remote application will capture and interpret the data, and then graph it for use by system administrators.

To configure Voice Quality Statistics Integration settings:

1. On the MBG main page, click the Teleworking tab and click Application integration.

2. Click to add a record.

3. In the V oice Quality Statistics Integrationframe, enter or edit the options as required and then click Save:

Field | Description
Address | Enter the IP address of the remote fault and performance monitoring application. MBG will send voice quality statistical data to this address.
UDP Port | Enter the UDP port number of the remote fault and performance monitoring application. MBG will send voice quality statistical data to this port.

Parent topic: Application Integration
↑