# Audio settings

Here you can specify a terminal's audio features.

Table 1. Ring settings
Parameter | Explanation
Ring off | Calls are not signalled acoustically.
Internal ring melody | The ring melody for internal calls is set here.
Use external melody | External calls are signalled by the external melody. External calls are signalled by the internal melody and external ring pattern.
External ring melody | The ring melody for external calls is set here.
Ring volume | Set the ring volume for internal and external ring melody here.
Ring speed | Set the ring speed for internal and external ring melody here.

Table 2. Volume
Parameter | Explanation
Loudspeaker volume | The loudspeaker volume is set on the phone here.
Handset volume | The loudspeaker volume is set on the handset here.

Table 3. Discreet ring - The phone rings only once.
Parameter | Explanation
Discreet ring | Discreet ring is enabled (The phone rings only once).
Discreet ring melody | Separate audio settings are available for discreet ring. Select here the melody, volume and speed of the discreet ring.
Discreet ring volume
Discreet ring speed

Table 4. DECT signalling on the cordless phones
Parameter | Explanation
Vibra call | Calls are also signalled using repeated vibration. Text, voice mail and callback messages are signalled using a single vibration.
System overload beep | Acoustic signalling indicating that all the real-time resources of the DECT system are seized.
Range beep | Acoustic signalling indicating that the cordless phone has reached the limit of the coverage range.

Table 5. Attention tone, acoustic signalling for call waiting, announcement, message.
Parameter | Explanation
Attention melody | Calls are also signalled using repeated vibration. Text, voice mail and callback messages are signalled using a single vibration.
Attention volume | Acoustic signalling indicating that all the real-time resources of the DECT system are seized.

## Copying the audio configuration to another terminal

To copy the entire audio configuration of a terminal to the same type of terminal, proceed as follows:

1. Choose the terminal whose audio configuration you wish to transfer.

2. Click the Copy button on the top left side.

   All opened, similar terminals are displayed. Checkboxes are visible on the left side.

3. Tick the boxes of the terminals to which you want to copy the audio configuration, then click the Apply button.

   The audio configuration is copied.

Parent topic: Putting telephones and terminals into operation
↑