# System reset

The communication server can be rebooted with a restart or reset to its default values using a first start.

## Restart of the communication server

A restart reboots the entire communication system. The configuration data is preserved.

Note:

- Never disconnect the communication server from the power supply to trigger a restart. This can result in data losses and prevent a restart.
- The restart is triggered immediately. All the active call and data connections are interrupted.

## First start of the communication server

A first start has the effect of resetting the communication server from scratch. The system-specific data such as the system ID, system type, sales channel, licence code, software generation and IP address of the system are preserved.

notes:

- The first start is triggered immediately. All the active call and data connections are interrupted.
- A first start deletes all the configuration data already stored and replaces it with the default values of the sales channel. Therefore, always create a backup before configuration data first start.

## First start and reset sales channel

With this function the sales channel and licence code are also deleted during first start. During the next start, you will be prompted for the sales channel and licence file. Note that the licence code in the licence file is dependent on the sales channel and that you can no longer use the existing licence code.

## Shutting down the communication server (Mitel 415/430 only)

Before disconnecting the communication server from the power supply, it must be shut down in a controlled manner. It then remains in a special Shutdown Mode for three minutes before it starts again automatically. Within these three minutes, the communication server can be disconnected from the power supply.

notes:

- Never disconnect the communication server from the power supply before it is in Shutdown mode. This can result in data losses and prevent a restart.
- The F0 LEDs blink in shutdown mode... F4 red and the SYS LED green.
- The shutdown is immediately triggered. All the active call and data connections are interrupted.

## Shutting down the communication server (Mitel 470 only)

Before disconnecting the communication server from the power supply, the Call Manager card (CPU1) and the application card (CPU2-S) must be shut down in a controlled manner. Both cards can be jointly or separately shut down via the control keys close to the display on Mitel 470.

notes:

- Never disconnect the communication server from the power supply before it is completely shut down (CPU1 and CPU2-S). This can result in data losses and prevent a restart.
- The call manager card (CPU1) can only be shut down via the control keys of the Mitel 470 display. The application card (CPU2-S) can also be shut down via WebAdmin.
- The shutdown is immediately triggered. All active call and data connections are interrupted, and all applications closed without warning the user.

## Shutting down and restarting application card (Mitel 470 only)

The operating system of the applications card is shut down regularly and the applications card is deactivated or restarted.

Note:

The shutdown is immediately triggered. All applications are closed without warning the user.

Parent topic: File management
↑