# Licence overview

All available licences and their most important features are listed here in groups.

Table 1. Software
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Software Release | Allows a particular software release to be operated | Restricted * | unrestricted | In the AIN, only on the Master; otherwise per node. |  |
* 4 hours after the new software is loaded, the communication server switches to a restricted operating mode.

Table 2. Users
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
User | Allows user operation on the communication server | Locked | 1, 20, 50 or 100 additional users per licence. | In the AIN, only on the Master; otherwise per node. |  |
IP User | Licence bundle: 1 additional user 8 phone licences (any type except Mitel One) 8 phones per user Video licence for all phones | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Entry UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Entry | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Standard UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Standard | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Premium UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Premium | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 3. Terminals
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
MiVoice 2380 IP Softphones | Number of registered MiVoice 2380 IP softphones | 0 | per licence 1 additional IP softphone | In the AIN, only on the Master; otherwise per node. |  |
MiVoice 5300 IP Phones | Number of registered , MiVoice 5360 IP, MiVoice 5361 IP, MiVoice5370 IP and MiVoice 5380 IP IP system phones | 0 | 1, 20 or 50 additional IP system phones per licence *The licences can also be used if the Mitel SIP Terminals licences are missing. | In the AIN, only on the Master; otherwise per node. |  |
Mitel SIP Terminals | Number of registered phones of the Mitel 6000 SIP series | 0 | 1, 20 or 50 additional Mitel SIP phone per licence | In the AIN, only on the Master; otherwise per node. |  |
Mitel 8000i Video Options | Use of the video functionality of a Mitel SIP phone | 0 | Additional licence for Mitel SIP Terminals. 1, 20 or 50 additional Mitel SIP phones with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |
Mitel Dialog 4200 Phones | Number of registered digital phones Dialog 4220, Dialog 4222 and Dialog 4223 on the Mitel 470 communication server | 0 | One additional phone per licence | In the AIN, only on the Master; otherwise per node. |  |
MMC Extensions | Number of mobile phones that can be registered with Mitel Mobile Client for operation with an Mitel Mobile Client Controller (MMCC) | 0 | per licence 1 additional mobile phone (with Mitel Mobile Client) | In the AIN, only on the Master; otherwise per node. |  |
Dual Homing | Number of registered Mitel 6000 SIP phones on a backup communication server | 0 | per licence 1, 20 or 50 additional phones | Always on the backup communication server |  |
Mobile or External Phone Extensions | Number of mobile phones that can be registered (without Mitel Mobile Client) | 0 | per licence 1 additional mobile phone (without Mitel Mobile Client) | In the AIN, only on the Master; otherwise per node. |  |
SIP Terminals | Number of registered standard SIP terminals | 0 | one additional standard SIP phone per licence | In the AIN, only on the Master; otherwise per node. |  |
Video Terminals | Use of the video functionality of a standard SIP terminal | 0 | Additional licence for SIP Terminals. 1 additional standard SIP terminal with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 4. BluStar
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
BluStar Softphones | Number of registered BluStar softphones | 0 | 1, 20 or 50 additional BluStar softphones | In the AIN, only on the Master; otherwise per node. |  |
BluStar Softphone Video Options | Use of the video functionality of a BluStar softphone | 0 | Additional licence for BluStar softphone. 1, 20 or 50 additional BluStar softphones with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 5. Audio services
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Conference Bridge (Dial-In Conference) | Use of conference bridge | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Number in Queue | Use of the function 'queue with announcement ' | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Auto Attendant | Use of the Auto Attendant function. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Enterprise Voice Mail | Voice compression, expanded voice memory capacity, and e-mail notification whenever new voice messages are received, forwarding of voice messages, call recording. | unavailable | Enabled (including 2 audio channels for voice mail, Auto Attendant or call recording) | In the AIN, only on the Master; otherwise per node. |  |
Audio Record & Play Channels | Voice channels for recording or playing back audio data. | unavailable | per licence 1 additional audio channel for voice mail, Auto Attendant or call recording | In the AIN, only on the Master; otherwise per node. |  |

Table 6. Features
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Analogue Modem | - | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Secure VoIP | Encrypted VoIP connections using SRTP and TLS. | Non-encrypted transmission | Encrypted transmission | per node |  |
Silent Intrusion | Using the Silent Intrusion feature. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |

Table 7. Resources
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Mitel SMBC Base licence (Mitel SMBC only) | Allows the operation of Mitel SMBC with 10 users. No additional licences needed for setting up a AIN. | Restricted | Unrestricted with up to 10 users (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
Mitel 470 Base licence (Mitel 470 only) | Allows the operation of Mitel 470 with 20 users. No additional licences needed for setting up a AIN. | Restricted | Unrestricted with up to 20 users (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
Base licence Virtual Appliance (Virtual Appliance only) | Allows the operation of Virtual Appliance. No additional licences needed for setting up a AIN. | Restricted | Unrestricted (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
VoIP Channels for Standard Media Switch* | VoIP functionality | 0 / 2** | Per licence 1 additional VoIP channel | In the AIN, only on the Master; otherwise per node. |  |
* If Virtual Appliance is used as Master, the VoIP channels of the master node are made available without a licence from the integrated Mitel Media Server. However, for the satellites' VoIP channels, the licences must be purchased. **If VoIP mode is set to G.711, two G.711 VoIP channels per system can be used without a licence.

Table 8. Network
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Lync Option for SIP Access Channels (Mitel 470 only) | Enables using a SIP access channel with Lync-specific options and features. | 0 | Additional licence for SIP Access Channels. Per licence one additional channel with Lync-specific options and features. | In the AIN, only on the Master; otherwise per node. |  |
B-Channels on PRI Cards | B channels that can be used simultaneously on the PRI interface card | 10 | Per licence 1 additional B- channel | In the AIN, only on the Master; otherwise per node. |  |
SIP Access Channels | Simultaneously usable channels to an SIP provider | 0 | Per licence 1 additional SIP access channel | In the AIN, only on the Master; otherwise per node. |  |

Table 9. Private networking
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
QSIG Networking Channels* | QSIG channels | 0 | per licence 4 or n QSIG channels (n limited by the system capacity) | per node |  |
*For Virtual Appliance this licence is only relevant to the QSIG networking of an AIN satellite.
Base Mitel AIN Mitel 430 only | Operation of an AIN | locked | AIN with master and one satellite | Only on the Master |  |
Mitel AIN Satellites Mitel 430 only | Additional satellite in an AIN | 0 | Additional licence for Base Mitel AIN. 1 additional satellite per licence | Only on the Master |  |

Table 10. Applications
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Advanced Messaging | SMPP protocol for integration of an SMS server and registration of 9d cordless phones. (Includes SMPP licence) | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
CTI First Party via LAN | First-party CTI clients with basic functions on Ethernet interface | 0 | enabled for a specific number of users. | In the AIN, only on the Master; otherwise per node. |  |
Dialers | Number of simultaneously active, user-linked Mitel Dialer applications. | 0 | 1, 20 or 50 additional instances per licence | In the AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Base (Mitel 470 only) | Send receive fax messages and configure users with fax mailboxes. | 0 | 2 licences CPU2 Fax Channelsand 10 licences CPU2 Fax Clients. | In AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Channels (Mitel 470 only) | Additional fax media channel. | 0 | 1 additional fax media channel per licence (max. 8) | In the AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Clients (Mitel 470 only) | Additional users with fax mailboxes. | 0 | 1, 20 or 50 additional fax mailboxes per licence | In the AIN, only on the Master; otherwise per node. |  |
Hospitality Manager | Use of Hospitality Manager | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Hospitality PMS Interface | Use of the PMS interface and therefore of the FIAS protocol. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Hospitality PMS Rooms | Number of rooms when using the PMS interface. | 0 | 1, 20, 50 or 100 rooms per licence | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Basic Package | Basic licence: Prerequisite for all other OpenCount licences. Enables connection to the MiVoice Office 400 and the use of basic functions. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Healthcare Branch Package | Additional licence: Offers extra functions for care homes and retirement homes. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Public Authorities Branch Package | Additional licence: Offers extra functions for municipalities, communities and ministries. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Functional Upgrade to Comfort | Additional licence: Offers extra functions such as PIN telephony. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Functional Upgrade to Premium | Additional licence: Offers extra functions such as intermediate statements, invoicing etc. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Users | Additional licence: Enables a defined number of users to be monitored via OpenCount. | 0 | 1, 20 or 50 additional users per licence | In the AIN, only on the Master; otherwise per node. |  |

Table 11. Interfaces
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
ATAS Interface | Use of the ATAS interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
ATASpro Interface | Use of the ATASpro interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
BSS Licence | Right to connect a BluStar server | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
BSS-Lync Interface | Right to use the BluStar Lync interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
CSTA Sessions | Number of monitored terminals via the CSTA protocol. | 0 | 1, 20, 50 or 100 CSTA sessions per licence | In the AIN, only on the Master; otherwise per node. |  |
Presence Sync. via SIMPLE and MSRP | Number of users who can use one (or both) protocols for the third-party applications. | 0 | 1, 20 or 50 additional users per licence who may use both protocols. | In the AIN, only on the Master; otherwise per node. |  |
OAI Interface | Use of the Open Application Interface | Locked | Enabled | In the AIN, only on the Master; otherwise per node. |  |

Parent topic: System configuration
↑