# IP network

Here you will find the IP network settings of the applications card.

Table 1. IP network adapter of the applications card: Designation and settings
Parameter | Explanation
--- | ---
Device | Name of the network adapter integrated on the applications card (read only).
MAC address | MAC address of the network adapter integrated on the applications card (read only).
DHCP enabled | DHCP is enabled (default value)
IP address / Subnet mask | IP address and subnet mask of the applications card. If DHCP is deactivated, the default value is 192.168.104.014. Note: If you disable DHCP and statically address the applications card, please note that the applications card IP address must be on the same subnet as the communication server IP address. Note: If you want to change the IP address of both the communication server AND the applications card, always change the IP address of the applications card first!
Gateway | Subnet standard gateway The default value 192.168.104.013. This is the standard IP address of the communication server.
Primary DNS | Here you can specify which DNS servers are queries in what sequence for resolving a name. If you are only using one DNS server, leave the entry for Secondary DNS blank.
Secondary DNS | The applications card is known under this name in this workgroup.

Parent topic: Multimedia
↑