# IP address / Location mapping

It is possible to map an IP address or an IP address range to an emergency location data set. This is useful for IP phones, SIP phones, or SIP-DECT radio units which have static locations.

The use of this table requires that the company’s IT department set up their network in a way, so that they know where each LAN cable ends. Further it is important, that this setup does not change. If it does, this mapping table has to be adapted accordingly.

## Mapping an IP address (range) to a emergency location data set

1. Click the symbol.

2. Enter the IP address in the first field.

3. If you want to map an address range, enter the IP address in the second field.

Note:

For a valid IP address range, the second IP address must be higher then the first one.

1. Select the suitable emergency location data set

2. Confirm with .

## Deleting an IP address mapping

To delete a IP address mapping, click the symbol.

See also...

## Focus topic

"Emergency service support"

Parent topic: Emergency calls
↑