# Exchange Connector

Lets you configure the administration access to the Exchange Connector of OIP.

Table 1. OIP Exchange configuration driver parameters
Parameter | Description
Microsoft Exchange Server Version | Select here the version of the Microsoft Exchange Server to be connected.
Download server address | Microsoft Exchange Server DNS name or IP address. If the network contains several Microsoft Exchange Servers, the IP address of the server defined in the Client Access Server (CAS) role must be indicated.
Domain name | Domain assigned to the Microsoft Exchange Server, for instance company.com.
User name | OIP Exchange administrator user.
Password | OIP Exchange administrator's password.
Notification interval | Interval during which the OIP Exchange driver checks the modifications on the Microsoft Exchange Server.
Log level | The log level needs to be set in case of OIP Exchange driver malfunction. The log level determines the number of inputs in the log file. The protocol files are written in the following directory, depending on the operating system: Windows XP: c:\Documents and Settings\All Users\Applications data\Aastra\Oip\MsxDrv\Log\ Windows Server 2008/2008 R2 and Windows 7/Vista: c:\ProgramData\Aastra\Oip\MsxDrv\Log\ The folder option Display hidden files, folders and drives must be selected to display the log files.
Log storage days | Number of days after which older protocol files are deleted.
Maximum protocol file size | Maximum protocol file size. A new protocol file is added after reaching the size.

Parent topic: Multimedia
↑