# Hotline destinations

Define up to 20 hotline destinations here and determine the dialling delay for each hotline destination.

A user can be assigned one of 20 different hotline destinations. Whenever the handset of a terminal assigned to the user is lifted, the configured hotline call number will automatically be dialled once the set delay has expired.

Note:

One hotline call number and a delay time can also be configured for each terminal. The configuration on the terminal takes precedence over the user configuration. If a hotline destination is configured for the terminal and user, the terminal hotline destination is called, regardless of the configured delays.

Parent topic: Mitel Mobile Client
↑