# Setting up SIP providers and accounts

(Configuration "Routing" Incoming view)

Here you can set up the access to an SIP provider if you want to implement the exchange line circuit via a VoIP connection to an SIP provider. Otherwise, you can skip this step.

First set up the SIP provider. Then open the SIP account for the SIP provider access.

Proceed as follows:

1. Click the Add button in the Network interfaces column.

   The Add SIP provider overlay view is opened.

2. Follow the instructions in the Assistant window.

   The SIP provider is now added and is displayed in the Network interfaces column.

3. Double-click the Network interfaces column on the box of the newly added SIP provider.

   The Overlay view SIP provider is opened.

4. Follow the instructions in the Assistant window.

   The SIP account and access to the SIP provider are now set.

Parent topic: Configuration assistant
↑