# IP addressing

Here you can see the IP addressing for your communication server.

Table 1. IP addressing
Parameter | Explanation
Host name | Host name of the communication server for the address allocation in the DNS server or via Multicast DNS (default entry: <Model name>-<MAC address>, for example “Mitel430-00085d8031a6”)
IP address | IP address of the communication server (default entry: "192.168.104.13").
Subnet mask | Default entry: “255.255.255.0”
Gateway | Default gateway of the communication server (default entry: “0.0.0.0”).
MAC address | MAC address of the communication server.

Table 2. CLIP/CLIR settings
Parameter | Explanation
DHCP client | The IP address is retrieved from the DHCP server and used in the communication server. The IP address is static and has to be entered manually.
Primary DNS server | Address of the primary DNS server (entry is read from the DNS server).
Secondary DNS server | Address of the secondary DNS server (entry is read from the DNS server).
Domain | Domain name (entry is read from the DNS server).
Multicast DNS support | Activates the integrated Multicast DNS Responder. SIP system phones need it to be able to find the communication server by themselves and register with it (default setting: ).

See also...

Least Cost Routing (LCR)

Parent topic: System configuration
↑