# International dialling tone

Up to 10 digit sequences can be defined here for the international dialling tone.

For analogue network interfaces up to 10 digit sequences can be defined for the international dialling tone. This can be assigned in the Call routing view for each network interface. If dialling starts with this digit sequence, the dialling process is interrupted in order to wait for the international dialling tone.

Parent topic: Multi site
↑