# DECT phones

Subscribed DECT phones are displayed here.

Table 1. DECT Phones parameters
Parameter | Description
Display name | Name of the user.
Number | User number.
IPEI | Unique identifier of each phone.
HW Type | Hardware type of the phone.
Subscribed | If a green tick mark is displayed, then the DECT phone is subscribed.
Download | Displays the progress of updating the handset firmware.
Version | Software version of the phone.

## Subscription of a new DECT phone

To subscribe to a new phone, under System - DECT phones, click the Switch on button.

Once the phone is subscribed, you can see a tick mark under Subscribed column confirming subscription for SIP-DECT terminal on RFP.

Important:

- The handset should have the SIP-DECT system as the “Download Over Air Master”. For this purpose, the handset should be registered to SIP-DECT system.
- Once all SIP-DECT phones have been subscribed, click the Switch off button. This prevents registration of further phones in the DECT system.

hints:

- We strongly recommend a user pin length of 4 digits.
- After subscription, the SIP-DECT handsets might need to upgrade their firmware. The upgrade happens automatically over the air in the background. This might take several hours.

## Searching for and displaying specific phones

To search and display specific phones, enter as filter criterion a string of characters contained in one or more columns and then click Filter button.

hint:

You can search from any of the parameter.

## Deleting one or more DECT phones

1. Under SIP-DECT - DECT phones button, click Delete. Check box is displayed in the beginning of the table to select the phone(s) to delete.

2. Click the Delete button.

Parent topic: TDM-DECT
↑