# Configuring AIN (guide)

This guide will help you configure an AIN. The entire AIN is configured via the Master as if it were a single communication server. The individual nodes are identified by their node numbers. Node 0 is always the Master. The satellites are numbered in the sequence in which they logged on to the Master. The complete port address is therefore Node 2 Port 0.10-1.

## Configuration tools

The following tools are available for the administration and configuration operations:

- The Mitel CPQ Project Manager is used for planning and drawing up quotations for an AIN.

- Use the WebAdmin administration access for configuration and administration.

- For user and call charge administration use the System Assistant access of WebAdmin.

## Configuring call routing and connection resources

1. First create or complete the basic data such as the direct dialling plan, numbering plan, users and abbreviated dialling lists

2. Configure the media resources according to the calculated values of the Mitel CPQ Project Manager.

3. Configure the node-specific settings for the AIN.

4. Configure the AIN regions in the Regions view.

5. If necessary, configure the bandwidth areas.

6. Configure the PSTN overflow in the PSTN overflow view.

7. Configure the routing for integrated mobile phones and PISN users (see System Manual MiVoice Office 400 Private Networking).

8. Configure the emergency number destinations for the AIN. Please note that nodes in other areas usually also have other emergency destinations. These nodes should have their own exchange accesses so that the emergency destinations can be dialled directly.

9. Configure the switch groups for the AIN.

## Configuring DECT system and other devices

1. Configure the DECT system.

   In regular AIN operation all the cordless phones are logged on to the Master. Users are able to use their cordless phones on the same call number in the radio area of each node without having to log on there specially (roaming).

   For Mitel 600 DECT: Configure the selected software update locally on the devices under the Download server. menu entry.

   For Office 135 and Office 160pro/Safeguard/ATEX: Log the cordless phones onto DECT system A to ensure that the software of the cordless phones is also updated whenever the Master software is updated.

2. Configure the other devices and features such as LCR, door intercom systems, music on hold or a voice mail system.

Parent topic: Product information
↑