# Licence overview

All available licences and their most important features are listed here in groups.

Table 1. System
Parameter | Explanation
Equipment ID (EID) | Identification number of the communication system.
Sales channel | Name of the designated sales channel.
Communication server | Type designation of the communication server.
Release | Release number.
Support ID | Communication server identification compared to the support. The support ID is generated on the licence server with the help of the EID and - after the first internet connection of the communication server with the licence server - entered here automatically.
Configured users | Number of configured users in the system. In brackets you find more detailed information about the type of the configured users.
User licences (used / available / total) | Overview of the used / available / total number of user licences including IP user licence bundles and UCC licence bundles.

Table 2. Subscription
Parameter | Explanation
State | Status of subscription.
Number | Subscription ID

Table 3. Licence (LIC)
Parameter | Description
License file | The licenses files is downloaded automatically. When the system has an active subscription, the automatic download is the only option. If there is no active subscription, the license file is uploaded manually using the Browse button.

Table 4. Software
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Software Release | Allows a particular software release to be operated | Restricted * | unrestricted | In the AIN, only on the Master; otherwise per node. |  |
* 4 hours after the new software is loaded, the communication server switches to a restricted operating mode.

Table 5. User Licences
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
User | Allows user operation on the communication server | Locked | 1, 20, 50 or 100 additional users per licence. | In the AIN, only on the Master; otherwise per node. |  |
IP User | Licence bundle: 1 additional user 8 phone licences (any type except Mitel One/MOMA/MOWA) 8 phones per user Video licence for all phones | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Entry UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Entry | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Standard UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Standard | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |
Premium UCC User | Licence bundle: 1 additional user 8 phone licences (any one) 8 phones per user Video licence for all licensed phones. MiCollab role UCC Premium | 0 | 1 additional user per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 6. Terminals
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
MiVoice 2380 IP Softphones | Number of registered MiVoice 2380 IP IP softphones | 0 | per licence 1 additional IP softphone | In the AIN, only on the Master; otherwise per node. |  |
MiVoice 5300 IP Phones | Number of registered , MiVoice 5360 IP, MiVoice 5361 IP, MiVoice 5370 IP and MiVoice 5380 IP IP system phones | 0 | 1, 20 or 50 additional IP system phones per licence *The licences can also be used if the Mitel SIP Terminals licences are missing. | In the AIN, only on the Master; otherwise per node. |  |
Mitel SIP Terminals | Number of registered phones of the Mitel 6000 SIP series | 0 | 1, 20 or 50 additional Mitel SIP phone per licence | In the AIN, only on the Master; otherwise per node. |  |
Mitel 8000i Video Options | Use of the video functionality of a Mitel SIP phone | 0 | Additional licence for Mitel SIP Terminals. 1, 20 or 50 additional Mitel SIP phones with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |
Mitel Dialog 4200 Phones | Number of registered digital phones Dialog 4220, Dialog 4222 and Dialog 4223 on the Mitel 470 communication server | 0 | One additional phone per licence | In the AIN, only on the Master; otherwise per node. |  |
MMC Extensions | Number of mobile phones that can be registered with Mitel Mobile Client for operation with an Mitel Mobile Client Controller (MMCC). Number of mobile phones that can be registered with Mitel One via the Mitel CloudLink platform. | 0 | per licence 1 additional mobile phone (with Mitel Mobile Client) | In the AIN, only on the Master; otherwise per node. |  |
Dual Homing | Number of registered Mitel 6000 SIP phones on a backup communication server | 0 | per licence 1, 20 or 50 additional phones | Always on the backup communication server |  |
Mobile or External Phone Extensions | Number of mobile phones that can be registered (without Mitel Mobile Client) | 0 | per licence 1 additional mobile phone (without Mitel Mobile Client) | In the AIN, only on the Master; otherwise per node. |  |
SIP Terminals | Number of registered standard SIP terminals | 0 | one additional standard SIP phone per licence | In the AIN, only on the Master; otherwise per node. |  |
Video Terminals | Use of the video functionality of a standard SIP terminal | 0 | Additional licence for SIP Terminals. 1 additional standard SIP terminal with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 7. BluStar
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
BluStar Softphones | Number of registered BluStar softphones | 0 | 1, 20 or 50 additional BluStar softphones | In the AIN, only on the Master; otherwise per node. |  |
BluStar Softphone Video Options | Use of the video functionality of a BluStar softphone | 0 | Additional licence for BluStar softphone. 1, 20 or 50 additional BluStar softphones with video functionality per licence. | In the AIN, only on the Master; otherwise per node. |  |

Table 8. Audio services
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Conference Bridge(Dial-In Conference) | Use of conference bridge | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Number in Queue | Use of the function 'queue with announcement ' | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Auto Attendant | Use of the Auto Attendant function. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Enterprise Voice Mail | Voice compression, expanded voice memory capacity, and e-mail notification whenever new voice messages are received, forwarding of voice messages, call recording. | unavailable | Enabled (including 2 audio channels for voice mail, Auto Attendant or call recording) | In the AIN, only on the Master; otherwise per node. |  |
Audio Record & Play Channels | Voice channels for recording or playing back audio data. | unavailable | per licence 1 additional audio channel for voice mail, Auto Attendant or call recording | In the AIN, only on the Master; otherwise per node. |  |

Table 9. Features
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Analogue Modem | - | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Secure VoIP | Encrypted VoIP connections using SRTP and TLS. | Non-encrypted transmission | Encrypted transmission | per node |  |
Silent Intrusion | Using the Silent Intrusion feature. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |

Table 10. Resources
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Mitel SMBC Base licence (Mitel SMBC only) | Allows the operation of Mitel SMBC with 10 users. No additional licences needed for setting up a AIN. | Restricted | Unrestricted with up to 10 users (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
Mitel 470 Base licence(Mitel 470 only) | Allows the operation of Mitel 470 with 20 users. No additional licences needed for setting up a AIN. | Restricted | Unrestricted with up to 20 users (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
Base licence Virtual Appliance(Virtual Appliance only) | Allows the operation of Virtual Appliance. No additional licences needed for setting up a AIN. | Restricted | Unrestricted (also in a AIN). | In the AIN, only on the Master; otherwise per node. |  |
VoIP Channels for Standard Media Switch* | VoIP functionality | 0 / 2** | Per licence 1 additional VoIP channel | In the AIN, only on the Master; otherwise per node. |  |
* If Virtual Appliance is used as Master, the VoIP channels of the master node are made available without a licence from the integrated Mitel Media Server. However, for the satellites' VoIP channels, the licences must be purchased. **If VoIP mode is set to G.711, two G.711 VoIP channels per system can be used without a licence.

Table 11. Network
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Lync Option for SIP Access Channels(Mitel 470 only) | Enables using a SIP access channel with Lync-specific options and features. | 0 | Additional licence for SIP Access Channels. Per licence one additional channel with Lync-specific options and features. | In the AIN, only on the Master; otherwise per node. |  |
B-Channels on PRI Cards | B channels that can be used simultaneously on the PRI interface card | 10 | Per licence 1 additional B- channel | In the AIN, only on the Master; otherwise per node. |  |
SIP Access Channels | Simultaneously usable channels to an SIP provider | 0 | Per licence 1 additional SIP access channel | In the AIN, only on the Master; otherwise per node. |  |

Table 12. Private networking
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
QSIG Networking Channels* | QSIG channels | 0 | per licence 4 or n QSIG channels (n limited by the system capacity) | per node |  |
*For Virtual Appliance this licence is only relevant to the QSIG networking of an AIN satellite.
Base Mitel AIN Mitel 430 only | Operation of an AIN | locked | AIN with master and one satellite | Only on the Master |  |
Mitel AIN Satellites Mitel 430 only | Additional satellite in an AIN | 0 | Additional licence for Base Mitel AIN. 1 additional satellite per licence | Only on the Master |  |

Table 13. Applications
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
Advanced Messaging | SMPP protocol for integration of an SMS server and registration of 9d cordless phones. (Includes SMPP licence) | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
CTI First Party via LAN | First-party CTI clients with basic functions on Ethernet interface | 0 | enabled for a specific number of users. | In the AIN, only on the Master; otherwise per node. |  |
Dialers | Number of simultaneously active, user-linked Mitel Dialer applications. | 0 | 1, 20 or 50 additional instances per licence | In the AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Base (Mitel 470 only) | Send/receive fax messages and configure users with fax mailboxes. | 0 | 2 licences CPU2 Fax Channels and 10 licences CPU2 Fax Clients. | In AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Channels (Mitel 470 only) | Additional fax media channel. | 0 | 1 additional fax media channel per licence (max. 8) | In the AIN, only on the Master; otherwise per node. |  |
CPU2 Fax Clients(Mitel 470 only) | Additional users with fax mailboxes. | 0 | 1, 20 or 50 additional fax mailboxes per licence | In the AIN, only on the Master; otherwise per node. |  |
Hospitality Manager | Use of Hospitality Manager | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Hospitality PMS Interface | Use of the PMS interface and therefore of the FIAS protocol. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Hospitality PMS Rooms | Number of rooms when using the PMS interface. | 0 | 1, 20, 50 or 100 rooms per licence | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Basic Package | Basic licence: Prerequisite for all other OpenCount licences. Enables connection to the MiVoice Office 400 and the use of basic functions. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Healthcare Branch Package | Additional licence: Offers extra functions for care homes and retirement homes. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Public Authorities Branch Package | Additional licence: Offers extra functions for municipalities, communities and ministries. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Functional Upgrade to Comfort | Additional licence: Offers extra functions such as PIN telephony. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Functional Upgrade to Premium | Additional licence: Offers extra functions such as intermediate statements, invoicing etc. | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
Mitel OpenCount Users | Additional licence: Enables a defined number of users to be monitored via OpenCount. | 0 | 1, 20 or 50 additional users per licence | In the AIN, only on the Master; otherwise per node. |  |

Table 14. Interfaces
Licence | Licensed attributes | Without licence | With licence | Licences for networking | Offline licence | Trial licence
ATAS Interface | Use of the ATAS interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
ATASpro Interface | Use of the ATASpro interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
BSS Licence | Right to connect a BluStar server | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
BSS-Lync Interface | Right to use the BluStar Lync interface | unavailable | enabled | In the AIN, only on the Master; otherwise per node. |  |
CSTA Sessions | Number of monitored terminals via the CSTA protocol. | 0 | 1, 20, 50 or 100 CSTA sessions per licence | In the AIN, only on the Master; otherwise per node. |  |
Presence Sync. via SIMPLE and MSRP | Number of users who can use one (or both) protocols for the third-party applications. | 0 | 1, 20 or 50 additional users per licence who may use both protocols. | In the AIN, only on the Master; otherwise per node. |  |
OAI Interface | Use of the Open Application Interface | Locked | Enabled | In the AIN, only on the Master; otherwise per node. |  |

Parent topic: System Overview
↑