# Coded ringing

A specific user can be searched for with the help of a coded call. Enter the user for the coded call here.

The installation of a general bell feature provides a paging system, albeit with a limited scope. Up to five internal users can be paged using a specific coded ringing on the general bell. A user who recognizes his ringing pattern can answer the call from any terminal.

The coded call consists of a longer tone and n subsequent shorter tones (n = 1...5 = Coded call ID).

Note:

The general bell is connected to an analogue terminal interface FXS. Precisely one FXS interface per communication server can be configured for this purpose (System / Interfaces / Analogue). Any existing allocation to a user is then automatically deleted. Once the connection is made, no calls can be made or received via the port.

Parent topic: Mitel Mobile Client
↑