# Configure IP Settings

The IP settings form is available if you are on the SMBC platform.

NOTE: It is strongly recommended to add a trusted network while configuring the LAN interface.

To configure the server name, do the following:

1. On the server manager, click IP settings under Configuration from the left menu.

2. Enter a Hostname. The default is mitel-networks-server.

## Internal Network Interface (LAN)

Complete the following to configure the LAN interface:

1. On the server manager, click IP settings under Configuration from the left menu. The IP addresses and hostname settings page opens.

2. In the Internal Network Interface (LAN) section, enter a unique IP address. This address must not be shared by any other devices

3. Enter a Second IP Address. This field is optional. The second IP address, if added, will be used as the LAN side IP of the MBG deployed in co-resident server gateway mode.

4. Enter the Netmask and the Gateway details. The netmask must match your existing networks.

5. Click Next. The Trusted Networks page opens.

## Reset Networks

This option is available only if the LAN IP address is already configured. Use the Reset Networks functionality to reset configurations to system default. See Reset Networks for more information.