# Reset Networks

The Reset Networks function deletes the LAN, the trusted networks, and the WAN configurations; and resets it to the default. Following a reset, you can access the server manager only by using the IP address configured for the SMB Controller Manager.

Do the following to reset networks to system default:

1. On the server manager, click IP settings under Configuration from the left menu.

2. Click Reset Networks. This option is available only if the LAN IP address is already configured.

3. Click Yes in the Confirm Reset Networks page. This deletes the LAN, the trusted networks, and the WAN configurations and restarts the system.

Note: Click No to cancel the reset action and return to the LAN configuration page.

After restart, the server manager can be accessed only using the IP address configured for the SMB Controller Manager.

Parent topic: IP Settings
↑