# SIP Trunk Status

Once a SIP trunk is configured and operational, the following metrics are displayed for it:

- Trunk Status:

- - Green check-mark - All trunks connected to both the ICPs and SIP service providers are "up."

  - Red x-mark - A trunking connection cannot be established between the ICPs and the SIP service providers.

- Reason - If a trunking connection cannot be established, a reason for the failure is provided.

- Calls in progress / Max - The number of calls currently in progress on the trunk, and the maximum number of calls that have been in progress on the trunk during the current session.

- Calls per hour / Max - The number of calls processed per hour on the trunk, and the maximum number of calls that have been processed per hour on the trunk during the current session.

To view the status of SIP trunks on MBG:

1. On the MBG main page, click the Service status tab and then click SIP Trunks.

2. To edit the trunk parameters, click beside the trunk you want to edit.

3. To reset the metrics, click Reset metrics beside the trunk you want to reset, and then click OK. The metrics (including maximum calls in progress and maximum calls per hour) will be returned to zero.