# Category 12: Give Messages Feature Bits

These feature bits control processing when users forward messages to single or multiple users, with or without additional comments. This category also contains receipt feature bits. This category does not allow users to send or broadcast messages marked “confidential.”

Bit | Description | Required | Incompatible
018 | Give and mark urgent | 024, 040 |
024 | Give messages (Master) | 040 |
025 | Give and request receipt | 024, 040 | 036
026 | Give to multiple destination | 024, 040 | 036
027 | Give and mark confidential | 024, 040 |
028 | Give with comments | 024, 040 |
033 | Give to user distribution list | 024, 040, 044 |
035 | Give to master distribution list | 024, 040, 045 |
061 | Wait to record | 022 or 026 |
084 | Give receipt message with comments | 040, 075, 086 |
085 | Give receipt message to multiple destinations | 024, 040, 086 |
086 | Give receipt message (Master) | 040 |
110 | Make/give to telephone number | 020 or 024, 040 |
126 | Make/give to mailbox with empty GCOS | 020, 040 |
157 | Repeat message for answering machine | 110 |
158 | Continue sending message | 020 or 024 or 029 |
192 | Give fax messages | 024, 190 |