# Search the Device List

You can search for one or more devices. Narrow your search using the following parameters:

- Sets per page — select the number of you wish to display.

- Enabled — specify what sort of devices to include in the search results: enabled, disabled or both enabled and disabled.

- type an entry in the Simple filter field to create a custom list of devices (see examples below)

Along with other device statistics, the number of entries in your search list is summarized at the bottom of each search result listing.

To search the device list:

1. On the MBG main page, click the Teleworking tab and click SIP or MiNet.

2. Define the search parameters:

   - Set per page—Enter the number of sets you wish to display on each page of the search list, 20, 50, 100, 500 or 1000.

   - Enabled—Specify whether you wish to view sets that are enabled, disabled, or both. Sets which are “enabled” on MBG can connect to the ICP (register).

   - Connected—Specify whether you wish to view sets that are connected, disconnected, or both connected and disconnected. Sets which are “connected” on MBG have successfully connected (registered) to the ICP.

   - Simple filter—Enter a search string to create the appropriate search listing, or clear the field to show all devices. See the simple search strings, below, for examples.

3. Click Refresh.

After completing a search of devices, you can then edit them simultaneously through the Bulk Modify feature.

Simple Search Strings

Use a simple search to find a device (or devices) by entering a Device ID, Description, DN, ICP Name, Time Zone or Cluster Zone.

Example 1:

- To locate a set with the DN number 1234, enter 1234.

Example 2:

- To locate sets on an ICP named ICP77, enter ICP77.

Parent topic: Managing Individual Devices